{"text_format":"1","workbook":"xlsx","n_sheets":15,"sheets":["BOM","LT3690 PS","PCB Mech","PIC Load Dump","WakeIn","WakeOut","LED Backlight","Prog","Analog Power Supply","Motor","Acoustic","LIN Xcvr","Ribbon Con","Block Cost","Components"],"not_rendered":{"charts":3,"images":15,"macros":1,"external_links":0,"defined_names":16,"comments":2,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM","index":0,"n_rows":91,"n_cols":22,"rows_kept":91,"cut":false,"hidden":false,"merged":[]}
["Subsystem","Manufacturer","Part Number","Qty","Designator","Description","Package","T-storage","Est. Cost","Qty","$ Ext.","Source","Length","Width","Height","Depth","Units","Length","Width","Height","Depth","Units"]
["+12v Supply",null,null,{"$f":"1+LEN(E2)-LEN(SUBSTITUTE(E2,\",\",\"\"))","v":1},"C13","0.68 uF on BOOST",null,null,0.15,null,{"$f":"D2*I2","v":0.15},null,null,null,null,null,null,{"$f":"IF(AND($Q2<>\"\",M2<>\"\"),M2*VLOOKUP($Q2,$A$70:$B$72,2),\"\")","v":""},{"$f":"IF(AND($Q2<>\"\",N2<>\"\"),N2*VLOOKUP($Q2,$A$70:$B$72,2),\"\")","v":""},{"$f":"IF(AND($Q2<>\"\",O2<>\"\"),O2*VLOOKUP($Q2,$A$70:$B$72,2),\"\")","v":""},{"$f":"IF(AND($Q2<>\"\",P2<>\"\"),P2*VLOOKUP($Q2,$A$70:$B$72,2),\"\")","v":""},{"$f":"IF(Q2<>\"\",IF(Q2=$A$72,$A$71,$A$72),\"\")","v":""}]
["+12v Supply",null,null,1,"C7","0.47 uF on VCCINT",null,null,0.15,null,{"$f":"D3*I3","v":0.15},null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,null,1,"C3","10 uF 75v",null,null,0.25,null,0.25,null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,null,1,"C14","100 uF 15v",null,null,0.35,null,0.35,null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,null,1,"C4","10 nF",null,null,0.05,null,0.05,null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,null,1,"C5","2.2 nF",null,null,0.05,null,0.05,null,null,null,null,null,null,"","","","",""]
["+12v Supply","On Semi","MBRS360BT3G",1,"D2","4A, 60v","SMB",null,0.29915999999999998,250,0.29915999999999998,"Digi-Key",8.1300000000000008,6.1,2.41,null,"mm",0.32007874015748033,0.24015748031496062,9.4881889763779537E-2,"","inch"]
["+12v Supply","Linear Tech","LT3690EUFE#PBF",1,"IC3","Switching P.S.",null,null,6.01,100,6.01,"Digi-Key",6,4,0.75,null,"mm",0.23622047244094488,0.15748031496062992,2.952755905511811E-2,"","inch"]
["+12v Supply",null,"R?",1,"R17","???R on VC",null,null,0.01,null,0.01,null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,null,1,"R21","73.2K, 0.1W, 1%",null,null,0.01,null,0.01,null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,null,1,"R22","38.3K, 0.1W, 1%",null,null,0.01,null,0.01,null,null,null,null,null,null,"","","","",""]
["+12v Supply",null,"R?",1,"R23","348K, 0.1W, 1%",null,null,0.01,null,0.01,null,null,null,null,null,null,"","","","",""]
["+12v Supply","TDK Corp","SLF12575T-470M2R7-H",1,"T1","47 uH, 2.7A (2.7A Sat)",null,null,0.82499999999999996,500,0.82499999999999996,"Digi-Key",12.5,12.5,7.5,null,"mm",0.49212598425196852,0.49212598425196852,0.29527559055118108,"","inch"]
["+12v Supply","Panasonic","ERJ-2RKF1003X",{"$f":"1+LEN(E15)-LEN(SUBSTITUTE(E15,\",\",\"\"))","v":1},"R31","100K, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,{"$f":"D15*I15","v":1.3639999999999999E-2},"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["+12v Supply","Panasonic","ERJ-2RKF1001X",{"$f":"1+LEN(E16)-LEN(SUBSTITUTE(E16,\",\",\"\"))","v":1},"R32","1K, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,{"$f":"D16*I16","v":1.3639999999999999E-2},"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["+12v Shutdown",null,null,1,"R5","???R, 0.1W, 1%","0402",null,0.01,null,0.01,null,1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["+12v Shutdown",null,null,1,"R6","???R, 0.1W, 1%","0402",null,0.01,null,0.01,null,1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["+12v Shutdown",null,null,1,"C1","0.1uF, 10v, 20%","0402",null,0.01,250,{"$f":"D19*I19","v":0.01},"Digi-Key",1,0.5,0.55000000000000004,null,"mm",3.937007874015748E-2,1.968503937007874E-2,2.1653543307086617E-2,"","inch"]
["+3.3v Supply","TDK Corp","C1005X5R1A104M",1,"C12","0.1uF, 10v, 20%","0402",null,1.3639999999999999E-2,250,1.3639999999999999E-2,"Digi-Key",1,0.5,0.55000000000000004,null,"mm",3.937007874015748E-2,1.968503937007874E-2,2.1653543307086617E-2,"","inch"]
["+3.3v Supply","Panasonic","EEE-1JA220UP",1,"C6","22uF 63v","CAN SMD",null,0.26,250,0.26,"Digi-Key",8,8,6.2,null,"mm",0.31496062992125984,0.31496062992125984,0.24409448818897639,"","inch"]
["+3.3v Supply","TDK Corp","C2012X7R2A104M",1,"C11","0.1uF, 100v, 20%","0805",null,7.4999999999999997E-2,250,7.4999999999999997E-2,"Digi-Key",2,1.25,1.45,null,"mm",7.874015748031496E-2,4.9212598425196846E-2,5.7086614173228342E-2,"","inch"]
["+3.3v Supply","NXP","BAS16,215",1,"D1","215mA, 100v, 250mW","SOT-23","-65, +150",4.752E-2,250,4.752E-2,"Digi-Key",3.04,2.64,1.22,null,"mm",0.11968503937007874,0.10393700787401575,4.8031496062992125E-2,"","inch"]
["+3.3v Supply","National","LM2936HVBMA-3.3",1,"IC2","3.3v Regulator","TO-252",null,1.54,250,1.54,"Digi-Key",9.6999999999999993,6.58,2.2999999999999998,null,"mm",0.38188976377952755,0.25905511811023624,9.0551181102362197E-2,"","inch"]
["Keypad","FCI","SFW8S-2STME1LF",1,"J2","8-pin flex cable connector","SMD",null,0.56620000000000004,250,0.56620000000000004,"Digi-Key",14.4,3.6,5.3,null,"mm",0.56692913385826771,0.14173228346456693,0.20866141732283464,"","inch"]
["Keypad","Fairchild","MMBT3904",2,"Q1,Q2","NPN, 200 mA, 40v, Beta 100","SOT-23","-55, +150",5.7320000000000003E-2,250,0.11464000000000001,"Digi-Key",3.04,2.64,1.22,null,"mm",0.11968503937007874,0.10393700787401575,4.8031496062992125E-2,"","inch"]
["Keypad","Panasonic","ERJ-2RKF2051X",1,"R7","2.050K 0.1W 1%","0402","-55, +125",1.3639999999999999E-2,250,1.3639999999999999E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["Keypad","Panasonic","ERJ-2RKF1001X",5,"R8,R9,R10,R11,R12","1.000K 0.1W 1%","0402","-55, +125",1.3639999999999999E-2,250,6.8199999999999997E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["Keypad","Panasonic","ERJ-2RKF3302X",1,"R13","33K, 0.1W, 1%","0402","-30, +100",1.3639999999999999E-2,250,{"$f":"D29*I29","v":1.3639999999999999E-2},"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["Keypad","Mallory","PK-12N40PQ",1,"SG1","Acoustic Signal, 4.1kHz, 3-15v, -20to90C",null,null,2.2058,100,2.2058,"Digi-Key",14,14,7.7,null,"mm",0.55118110236220474,0.55118110236220474,0.30314960629921262,"","inch"]
["Keypad","Taiyo Yuden","UMK105B7102KV-F",5,"C19,C20,C21,C22,C23","1000PF 50V 10%","0402",null,7.7999999999999996E-3,250,3.9E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["LIN","TDK Corp","C2012X7R2A104M",1,"C15","0.1uF, 100v, 20%","0805",null,7.4999999999999997E-2,250,7.4999999999999997E-2,"Digi-Key",2,1.25,1.45,null,"mm",7.874015748031496E-2,4.9212598425196846E-2,5.7086614173228342E-2,"","inch"]
["LIN","TDK Corp","C1608C0G2A221J",1,"C16","220pF, 100v, 5%","0603",null,3.9E-2,250,3.9E-2,"Digi-Key",1.6,0.8,0.95,null,"mm",6.2992125984251968E-2,3.1496062992125984E-2,3.7401574803149602E-2,"","inch"]
["LIN","NXP","BAS16,215",{"$f":"1+LEN(E34)-LEN(SUBSTITUTE(E34,\",\",\"\"))","v":1},"D3","215mA, 100v, 250mW (DO NOT POPULATE)","SOT-23","-65, +150",4.752E-2,250,{"$f":"D34*I34","v":4.752E-2},"Digi-Key",3.04,2.64,1.22,null,"mm",0.11968503937007874,0.10393700787401575,4.8031496062992125E-2,"","inch"]
["LIN","NXP","BZX84-B27,215",1,"D4","27v Zener","SOT-23","-65, +150",7.8640000000000002E-2,250,7.8640000000000002E-2,"Digi-Key",3.04,2.64,1.22,null,"mm",0.11968503937007874,0.10393700787401575,4.8031496062992125E-2,"","inch"]
["LIN","Infineon","TLE7259-2GU",1,"IC4","LIN Transceiver","8-SOIC",null,1.2693000000000001,100,1.2693000000000001,"Digi-Key",5,6,1.75,null,"mm",0.19685039370078738,0.23622047244094488,6.8897637795275593E-2,"","inch"]
["LIN","Fairchild","MMBT3904",1,"Q3","NPN, 200 mA, 40v, Beta 100","SOT-23","-55, +150",5.7320000000000003E-2,250,{"$f":"D37*I37","v":5.7320000000000003E-2},"Digi-Key",3.04,2.64,1.22,null,"mm",0.11968503937007874,0.10393700787401575,4.8031496062992125E-2,"",{"$f":"IF(Q37<>\"\",IF(Q37=$A$72,$A$71,$A$72),\"\")","v":"inch"}]
["LIN","Infineon","BSS123 L6327",1,"Q4","N-channel MOSFET","SOT-23","-55, +150",0.1512,100,0.1512,"Digi-Key",3.04,2.64,1.22,null,"mm",0.11968503937007874,0.10393700787401575,4.8031496062992125E-2,"","inch"]
["LIN","Panasonic","ERJ-2RKF1003X",1,"R24","100K, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,1.3639999999999999E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["LIN","Stackpole","RNCP1206FTD2K00",{"$f":"1+LEN(E40)-LEN(SUBSTITUTE(E40,\",\",\"\"))","v":2},"R25, R36","2K, 0.5W, 1% (DO NOT POPULATE)","1206",null,2.0160000000000001E-2,250,{"$f":"D40*I40","v":4.0320000000000002E-2},"Digi-Key",3.1,1.5,0.6,null,"mm",0.12204724409448819,5.905511811023622E-2,2.3622047244094488E-2,"","inch"]
["LIN",null,null,1,"R27","R?",null,null,0.01,null,0.01,null,null,null,null,null,null,"","","","",""]
["LIN",null,null,1,"R28","R?",null,null,0.01,null,0.01,null,null,null,null,null,null,"","","","",""]
["Micro","TDK Corp","C1005X5R1A104M",1,"C2","0.1uF, 10v, 20%","0402",null,1.3639999999999999E-2,250,1.3639999999999999E-2,"Digi-Key",1,0.5,0.4,null,"mm",null,null,null,null,"inch"]
["Micro","Microchip","PIC18F25K22-E/SO-ND",1,"IC1","PIC Microprocessor","SOIC-28","-65, +150",2.08,300,2.08,"Digi-Key",17.899999999999999,10.3,2.65,null,"mm",{"$f":"IF(AND($Q44<>\"\",M44<>\"\"),M44*VLOOKUP($Q44,$A$70:$B$72,2),\"\")","v":0.70472440944881887},{"$f":"IF(AND($Q44<>\"\",N44<>\"\"),N44*VLOOKUP($Q44,$A$70:$B$72,2),\"\")","v":0.40551181102362205},{"$f":"IF(AND($Q44<>\"\",O44<>\"\"),O44*VLOOKUP($Q44,$A$70:$B$72,2),\"\")","v":0.10433070866141732},{"$f":"IF(AND($Q44<>\"\",P44<>\"\"),P44*VLOOKUP($Q44,$A$70:$B$72,2),\"\")","v":""},"inch"]
["Micro","Sullins","NPPC071KFXD",1,"J1","7-Pin Programming connector",null,null,0.64400000000000002,250,0.64400000000000002,"Digi-Key",18.28,2.5,7.1,null,"mm",0.71968503937007877,9.8425196850393692E-2,0.27952755905511811,"","inch"]
["Micro","Panasonic","ERJ-8GEYJ101V",1,"R4","100R 1/4W 5%","1206","-55, +125",1.3639999999999999E-2,250,1.3639999999999999E-2,"Digi-Key",3.2,1.6,0.7,null,"mm",0.12598425196850394,6.2992125984251968E-2,2.7559055118110232E-2,"","inch"]
["Motor","TDK Corp","C2012X7R2A104M",1,"C18","0.1uF, 100v, 20%","0805",null,7.4999999999999997E-2,250,7.4999999999999997E-2,"Digi-Key",2,1.25,null,null,"mm",7.874015748031496E-2,4.9212598425196846E-2,"","","inch"]
["Motor","Infineon","TLE5205-2G",1,"IC5","H-Bridge","TO-263",null,5.4107000000000003,100,5.4107000000000003,"Digi-Key",15,10,4.4000000000000004,null,"mm",0.59055118110236215,0.39370078740157477,0.17322834645669294,"","inch"]
["Motor","Mabuchi","FC280SC-20150",1,"Motor","Motor",null,null,1.95,100,1.95,"Kysan",45,24.2,18.3,null,"mm",1.7716535433070866,0.952755905511811,0.72047244094488194,"","inch"]
["Motor","Panasonic","ERJ-2RKF4751X",{"$f":"1+LEN(E50)-LEN(SUBSTITUTE(E50,\",\",\"\"))","v":1},"R26","75K, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,1.3639999999999999E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["Sense","TDK Corp","C1005X7S2A103K",3,"C8,C9,C10","0.01uF 60v","0402","-55, +125",2.9239999999999999E-2,250,8.7719999999999992E-2,"Digi-Key",1,0.5,0.55000000000000004,null,"mm",3.937007874015748E-2,1.968503937007874E-2,2.1653543307086617E-2,"","inch"]
["Sense","Panasonic","ERJ-2RKF1003X",3,"R14,R15,R16","100K, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,4.0919999999999998E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["Sense","Panasonic","ERJ-2RKF8871X",3,"R18,R19,R20","8870R, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,4.0919999999999998E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
["Sense","Panasonic","ERJ-8GEYJ562V",2,"R34,R35","5.6K, 0.25W, 5%","1206","-55, +125",1.3639999999999999E-2,250,2.7279999999999999E-2,"Digi-Key",3.2,1.6,0.7,null,"mm",0.12598425196850394,6.2992125984251968E-2,2.7559055118110232E-2,"","inch"]
["Wake Out","TDK Corp","C2012X7R2A104M",1,"C17","0.1uF, 100v, 20%","0805",null,7.4999999999999997E-2,250,7.4999999999999997E-2,"Digi-Key",2,1.25,1.45,null,"mm",7.874015748031496E-2,4.9212598425196846E-2,5.7086614173228342E-2,"","inch"]
["Wake Out","Infineon","BSP452",1,"IC6","High side switch","SOT-223",null,1.4280999999999999,100,1.4280999999999999,"Digi-Key",6.5,7,1.7,null,"mm",0.25590551181102361,0.27559055118110237,6.6929133858267709E-2,"","inch"]
["Development","Panasonic","LNJ308G8LRA",3,"LED1, LED2, LED3","Green LEDs (-30 to +85)","0603",null,0.13900000000000001,250,0.41700000000000004,"Digi-Key",1.6,0.8,0.8,null,"mm",6.2992125984251968E-2,3.1496062992125984E-2,3.1496062992125984E-2,"","inch"]
["Development","Panasonic","ERJ-2RKF1820X",3,"R1,R2, R3","182R, 0.1W, 1%","0402","-55, +125",1.3639999999999999E-2,250,4.0919999999999998E-2,"Digi-Key",1,0.5,0.4,null,"mm",3.937007874015748E-2,1.968503937007874E-2,1.5748031496062992E-2,"","inch"]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,"","","","",""]
[]
[null,null,null,null,null,null,null,null,null,"Total",{"$f":"SUM(K2:K66)","v":27.339139999999997}]
[]
[]
["Unit Lookup","To alternate"]
["inch",{"$f":"1/B72","v":25.4}]
["mm",{"$f":"1/25.4","v":3.937007874015748E-2}]
[]
[]
[]
[]
[]
[]
[]
[]
["Row Labels","Sum of Est. Cost"]
["+12v Supply",7.1341599999999996]
["+3.3v Supply",1.9361600000000001]
["Keypad",2.3186]
["LIN",1.4824600000000003]
["Micro",2.1072800000000003]
["Motor",7.4493400000000003]
["Sense",5.6520000000000001E-2]
["Wake Out",1.5030999999999999]
["(blank)"]
["Grand Total",23.987619999999996]

{"sheet":"LT3690 PS","index":1,"n_rows":47,"n_cols":6,"rows_kept":47,"cut":false,"hidden":false,"merged":[]}
["Signal","Value","Units","Notes",null,"Based on LT3690"]
["V-IN",24,"v","Typical V-in"]
["V-IN Max",36,"v","Overload shutdown"]
[]
["V-OUT Target",8,"v"]
["Vin Low",9,"v"]
["RT [R21]",72900,"ohms"]
["R4 (FB to Gnd - R22)",38300,"ohms","R4 is data sheet reference"]
["R3 (Out to FB - R23)",{"$f":"B8*(V_OUT/V_FB-1)","v":344700},"ohms","R3 is data sheet reference"]
[{"$f":"A8 & \" => 1%\"","v":"R4 (FB to Gnd - R22) => 1%"},{"$f":"Resistor((B8))","v":38300},"ohms","Selected Resistor Value"]
[{"$f":"A9 & \" => 1%\"","v":"R3 (Out to FB - R23) => 1%"},{"$f":"Resistor((B9))","v":348000},"ohms","Selected Resistor Value"]
[{"$f":"A7 & \" => 1%\"","v":"RT [R21] => 1%"},{"$f":"Resistor((RT))","v":73200},"ohms","Selected Resistor Value"]
["V-FB",0.8,"v"]
["V-SW",0.37,"v"]
["V-LS",0.12,"v"]
["T-ON(min)",0.25,"usec"]
["T-OFF(min)",0.21,"usec"]
["Fsw(max)",{"$f":"(V_OUT+V_LS)/(0.000001*T_ON*(V_IN-V_SW+V_LS))/1000000","v":1.3675789473684212},"MHz","Highest acceptible frequency"]
["Freq (Select)",{"$f":"VLOOKUP(RT,A33:B47,2)","v":0.3},"MHz","Chosen frequency"]
["DC-min",{"$f":"F_Select*0.000001*T_ON*1000000","v":7.4999999999999997E-2},"% duty cycle"]
["DC-max",{"$f":"1-1000000*F_Select*0.000001*T_OFF","v":0.93700000000000006},"% duty cycle"]
["V-IN(min)",{"$f":"(V_OUT+V_LS)/(1-1000000*F_Select*0.000001*T_OFF)-V_LS+V_SW","v":8.9159551760939149},"v by duty cycle"]
["V-IN(max)",{"$f":"(V_OUT+V_LS)/(1000000*F_Select*0.000001*T_ON)-V_LS+V_SW","v":108.51666666666667},"v by duty cycle"]
["I-L(peak)",{"$f":"8+(V_IN_OVERLOAD-V_OUT)/(0.000001*Inductance)*0.000001*T_ON","v":8.3860010293360787},"A"]
["L - Inductor",{"$f":"(V_OUT+V_LS)*0.67/F_Select","v":18.134666666666664},"uHenry","Target Value"]
["Lmin - Inductor (min)",{"$f":"(V_OUT +V_LS)*0.42/F_Select","v":11.367999999999999},"uHenry","Minimum value"]
["I-L(Peak to peak ripple)",{"$f":"(1-10%)*(V_OUT+V_LS)/(B25*F_SW)","v":0.29467042864495258},"A"]
["C-OUT (output cap)",{"$f":"150/(V_OUT*F_SW)","v":13.710360221674875},"uF","(X5R or X7R ceramic best) or Electrolytic with ESR <= 0.03ohm"]
["C-Soft Start",{"$f":"B28/10000","v":1.3710360221674876E-3},"uF"]
["T-Ramp",{"$f":"B29*0.8/0.000002","v":548.41440886699513},"usec"]
[]
["Rt","MHz"]
[9590,1.5]
[10600,1.4]
[11800,1.3]
[13300,1.2]
[15000,1.1000000000000001]
[17000,1]
[19600,0.9]
[22700,0.8]
[26800,0.7]
[32400,0.6]
[40200,0.5]
[52200,0.4]
[72900,0.3]
[117000,0.2]
[164000,0.15]

{"sheet":"PCB Mech","index":2,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["Origin for PCB","Lower left corner",null,"from 5 Jan 2012 email",null,null,null,null,null,null,"Values","mm","Value","in"]
["PCB width",1.179,"in",null,null,null,null,null,null,null,25.4,"mm",{"$f":"K2/25.4","v":1},"in","test"]
["PCB height",3.25,"in",null,null,null,null,null,null,null,4.0339999999999998,"mm",{"$f":"K3/25.4","v":0.15881889763779528},"in","Ledge Diameter"]
["Hole 1 x (bottom left)",{"$f":"B2/2-0.315","v":0.27450000000000002},null,null,null,null,null,null,null,null,2.7330000000000001,"mm",0.10759842519685041,"in","Post Diameter"]
["Hole 1 y",{"$f":"(B3-2.972)/2","v":0.13900000000000001},null,null,null,null,null,null,null,null,5,"mm",0.19685039370078741,"in","Ramp width"]
["Hole 2 x (top-left)",{"$f":"B4","v":0.27450000000000002},null,null,null,null,null,null,null,null,25.637,"mm",1.0093307086614174,"in","lower post to lower diag rib"]
["Hole 2 y",{"$f":"B5+2.972","v":3.1109999999999998},null,null,null,null,null,null,null,null,3.262,"mm",0.12842519685039372,"in",{"$f":"1.139+0.128","v":1.2669999999999999}]
["Hole 3 x (top-right)",{"$f":"B4+0.6299","v":0.90440000000000009},null,null,null,null,null,null,null,null,23.95,"mm",0.94291338582677164,"in",{"$f":"3.111-M8","v":2.1680866141732285}]
["Hole 3 y",{"$f":"B7","v":3.1109999999999998},null,null,null,null,null,null,null,null,12.9,"mm",0.50787401574803159,"in"]
["Hole 4 x (bottom-right)",{"$f":"B8","v":0.90440000000000009}]
["Hole 4 y",{"$f":"B5","v":0.13900000000000001}]
["notch 1 x (center)",{"$f":"B2/2-0.646","v":-5.6499999999999995E-2}]
["notch 1 y",2.3250000000000002]
["notch 2 x",{"$f":"B2/2+0.648","v":1.2375}]
["notch 2 y",{"$f":"B13","v":2.3250000000000002}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"image is not quite symmetrical"]

{"sheet":"PIC Load Dump","index":3,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["Signal","Value","Units","Notes",null,"VDD","DAC Count","DAC V","Equiv Bat"]
["Battery",32,"v",null,null,3.3,0,{"$f":"($F$2*G2/2^5)","v":0},{"$f":"H2*($B$3+$B$4)/$B$4","v":0}]
["R16",100000,"ohm",null,null,null,1,0.10312499999999999,{"$f":"H3*($B$3+$B$4)/$B$4","v":1.2657518320180383}]
["R20",8870,"ohm",null,null,null,2,0.20624999999999999,{"$f":"H4*($B$3+$B$4)/$B$4","v":2.5315036640360766}]
["V analog in",{"$f":"B2*B4/(B3+B4)","v":2.6071461375952971},"v",null,null,null,3,0.30937499999999996,3.7972554960541141]
["V Ref",3.3,"v",null,null,null,4,0.41249999999999998,5.0630073280721533]
["A/D",{"$f":"B5/B6*2^12","v":3236.0213877546475},"Counts",null,null,null,5,0.515625,6.3287591600901916]
[null,null,null,null,null,null,6,0.61874999999999991,7.5945109921082281]
["R16 Nearest 1%",{"$f":"Resistor(B3)","v":100000},"ohm",null,null,null,7,0.72187499999999993,8.8602628241262682]
["R20 Nearest 1%",{"$f":"Resistor((B4))","v":8870},"ohm",null,null,null,8,0.82499999999999996,10.126014656144307]
[null,null,null,null,null,null,9,0.92812499999999998,11.391766488162345]
[null,null,null,null,null,null,10,1.03125,12.657518320180383]
[null,null,null,null,null,null,11,1.1343749999999999,13.92327015219842]
[null,null,null,null,null,null,12,1.2374999999999998,15.189021984216456]
[null,null,null,null,null,null,13,1.340625,16.4547738162345]
[null,null,null,null,null,null,14,1.4437499999999999,17.720525648252536]
[null,null,null,null,null,null,15,1.546875,18.986277480270576]
[null,null,null,null,null,null,16,1.65,20.252029312288613]
[null,null,null,null,null,null,17,1.7531249999999998,21.51778114430665]
[null,null,null,null,null,null,18,1.85625,22.78353297632469]
[null,null,null,null,null,null,19,1.9593749999999999,24.04928480834273]
[null,null,null,null,null,null,20,2.0625,25.315036640360766]
[null,null,null,null,null,null,21,2.1656249999999999,26.580788472378806]
[null,null,null,null,null,null,22,2.2687499999999998,27.846540304396839]
[null,null,null,null,null,null,23,2.3718749999999997,29.112292136414879]
[null,null,null,null,null,null,24,2.4749999999999996,30.378043968432912]
[null,null,null,null,null,null,25,2.578125,31.64379580045096]
[null,null,null,null,null,null,26,2.6812499999999999,32.909547632469]
[null,null,null,null,null,null,27,2.7843749999999998,34.175299464487033]
[null,null,null,null,null,null,28,2.8874999999999997,35.441051296505073]
[null,null,null,null,null,null,29,2.9906249999999996,36.706803128523106]
[null,null,null,null,null,null,30,3.09375,37.972554960541153]
[null,null,null,null,null,null,31,3.1968749999999999,39.238306792559186]

{"sheet":"WakeIn","index":4,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Signal","Value","Units","Notes"]
["Battery",36,"v"]
["R34",5600,"ohm","Parallel resistors to handle the power"]
["R35",5600,"ohm"]
["Current R34",{"$f":"$B$2/B3","v":6.4285714285714285E-3},"A"]
["Current R35",{"$f":"$B$2/B4","v":6.4285714285714285E-3},"A"]
["Power R34",{"$f":"$B$2*B5","v":0.23142857142857143},"W","0.25W"]
["Power R35",{"$f":"$B$2*B6","v":0.23142857142857143},"W"]
[null,null,null,null,{"$f":"12/0.004","v":3000}]
["Battery (low)",12,"v"]
["Load",{"$f":"1/(1/B3+1/B4)","v":2800},"ohm"]
["WakeIn current",{"$f":"B10/B11","v":4.2857142857142859E-3},"a"]
[]
[]
["R16 Nearest 1%",{"$f":"Resistor(B3, 10)","v":5620},"ohm"]
["R20 Nearest 1%",{"$f":"Resistor(B4)","v":5620},"ohm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"JD Requirement - 4 mA @ 12v for contact cleaning"]

{"sheet":"WakeOut","index":5,"n_rows":6,"n_cols":22,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Subsystem","Manufacturer","Part Number","Qty","Designator","Description","Package","T-storage","Est. Cost","Qty","$ Ext.","Source","Length","Width","Height","Depth","Units","Length","Width","Height","Depth","Units"]
[]
["Wake Out","Infineon","BSP452",{"$f":"1+LEN(E3)-LEN(SUBSTITUTE(E3,\",\",\"\"))","v":1},"IC6","High side switch","SOT-223",null,1.4280999999999999,100,{"$f":"D3*I3","v":1.4280999999999999},"Digi-Key",6.5,7,1.7,null,"mm",{"$f":"IF(AND($Q3<>\"\",M3<>\"\"),M3*VLOOKUP($Q3,$A$67:$B$69,2),\"\")","v":{"$error":"#N/A"}},{"$f":"IF(AND($Q3<>\"\",N3<>\"\"),N3*VLOOKUP($Q3,$A$67:$B$69,2),\"\")","v":{"$error":"#N/A"}},{"$f":"IF(AND($Q3<>\"\",O3<>\"\"),O3*VLOOKUP($Q3,$A$67:$B$69,2),\"\")","v":{"$error":"#N/A"}},{"$f":"IF(AND($Q3<>\"\",P3<>\"\"),P3*VLOOKUP($Q3,$A$67:$B$69,2),\"\")","v":""},{"$f":"IF(Q3<>\"\",IF(Q3=$A$69,$A$68,$A$69),\"\")","v":0}]
[]
["Wake Out","Infineon","BTS4140N",{"$f":"1+LEN(E5)-LEN(SUBSTITUTE(E5,\",\",\"\"))","v":1},"IC6","high side driver","SOT-223",null,0.93440000000000001,100,{"$f":"D5*I5","v":0.93440000000000001},"Digi-Key"]
["Wake Out","Infineon","BSS123 L6327",{"$f":"1+LEN(E6)-LEN(SUBSTITUTE(E6,\",\",\"\"))","v":1},null,"N-channel mosfet","SOT-23",null,0.1512,100,{"$f":"D6*I6","v":0.1512},"Digi-Key"]

{"sheet":"LED Backlight","index":6,"n_rows":35,"n_cols":5,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
["LEDs tied to 12v supply","Value","Units",null,"Notes"]
["LED Current at 12v",1.4999999999999999E-2,"A"]
["Number LEDs",5,"qty"]
["Q2 collector current",{"$f":"B2*B3","v":7.4999999999999997E-2}]
["Q2 Beta",50,"Beta"]
["Q2 Base Drive",{"$f":"B4/B5","v":1.5E-3},"A"]
["Q2 Vbe",0.6,"v"]
["Port Pin Vout High",3.1,"v"]
["R14 Base Drive resistor",{"$f":"(B8-B7)/B6","v":1666.6666666666667},"ohm"]
["Nearest 1% value",{"$f":"Resistor((B9))","v":1650},"ohm"]
["R14 Power dissipation",{"$f":"(B8-B7)*B6","v":3.7499999999999999E-3},"W"]
[]
[]
[null,null,null,null,"Touch Panel Manufacturer and TriMark have not yet current requirements"]
[]
["Development LEDs","Value","Units"]
["LED Drive voltage",3.3,"v"]
["LED voltage drop max",2.4,"v"]
["LED drive current",5.0000000000000001E-3,"A"]
["Series Resistor",{"$f":"(B17-B18)/B19","v":179.99999999999997},"ohm"]
["Nearest 1% value",{"$f":"Resistor(B20)","v":178},"ohm"]
["Resistor Power dissipation",{"$f":"(B17-B18)*B19","v":4.4999999999999997E-3},"W"]
[]
[]
[null,"Value","Units"]
["LED Voltage Drop",3.2,"v"]
["LED Max Current",0.02,"A"]
["# LEDs in Series",2,"pc"]
["Resistance - Series",130,"ohm"]
["Voltage - Minimum",9,"v"]
["Voltage - Maximum",32,"v"]
[]
[]
["Current at Vmin",{"$f":"(B30-B$28*B$26)/B$29","v":1.9999999999999997E-2},"A"]
["Current at Vmax",{"$f":"(B31-B$28*B$26)/B$29","v":0.19692307692307692},"A"]

{"sheet":"Prog","index":7,"n_rows":4,"n_cols":3,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Reset protection","Value","Units"]
["Series Resistor",100,"ohm"]
["Max voltage diff",5,"v"]
["Resistor Power Diss",{"$f":"B3^2/B2","v":0.25},"W"]

{"sheet":"Analog Power Supply","index":8,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["Description","Value","Units","Notes"]
["LM2936DT-3.3",3.3,"v","regulated output voltage, 50 mA max. -50, +60"]
[]
["V Battery min",9,"v"]
["V Battery max operating",32,"v","max operating (does not subtract reverse diode"]
["V Battery max",36,"v","auto-sleep"]
[]
["I Load min",0.5,"mA"]
["I Load max operating",12,"mA","Average current"]
["I Load max",2,"mA"]
[]
[]
["Power dissipation min",{"$f":"(B4-$B$2)*B8","v":2.85},"mW"]
["Power dissipation max oper.",{"$f":"(B5-$B$2)*B9","v":344.4},"mW","max operating"]
["Power dissipation max",{"$f":"(B6-$B$2)*B10","v":65.400000000000006},"mW","Linear regulator dissipation"]
[null,null,null,null,"Diode Drop",1,"v"]
["Ambient temp nominal",25,"°C",null,"Current",0.05,"A"]
["Ambient temp max",85,"°C",null,"Diode Power",{"$f":"1000*F16*F17","v":50},"mW"]
[]
[]
["Temp Rise J-A",140,"°C / W","Component spec"]
[]
["Calc. Temp Rise",{"$f":"B21*B14/1000","v":48.216000000000001},"°C"]
["Calc. Temp max oper",{"$f":"B18+B23","v":133.21600000000001},"°C","Spec is 150°C, with power diss internally limited"]
[]
[]
["Current Requirements","Value","Units"]
["PIC",5,"mA"]
["LED Driver",{"$f":"1000*(B2-0.6)/2050","v":1.3170731707317072},"mA"]
["Acoustic Driver",{"$f":"1000*(B2-0.6)/33000","v":8.1818181818181804E-2},"mA"]
["Test Point Drivers (3)",{"$f":"3*1000*(B2-1.6)/1080","v":4.7222222222222214},"mA"]
["HV Enable",{"$f":"1000*B2/100000","v":3.3000000000000002E-2},"mA"]
["LIN RxD",{"$f":"1000*B2/100000","v":3.3000000000000002E-2},"mA"]
["Total",{"$f":"SUM(B28:B33)","v":11.187113574772109},"mA"]

{"sheet":"Motor","index":9,"n_rows":29,"n_cols":4,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Description","Value","Units","Notes"]
["Min Voltage",9,"V","Assumes the motor is rated to operate at this minimum voltage"]
["Motor Current @Min V",5,"A","And current"]
["Power Min",{"$f":"B2*B3","v":45},"W"]
[]
["Voltage 1",12,"V"]
["Motor Current @V1",{"$f":"B$3 * B6/B$2","v":6.666666666666667},"A"]
["Power 1",{"$f":"B6*B7","v":80},"W"]
[]
["Voltage 2",24,"V"]
["Motor Current @V2",{"$f":"B$3 * B10/B$2","v":13.333333333333334},"A"]
["Power 2",{"$f":"B10*B11","v":320},"W"]
[]
["Voltage 2",32,"V"]
["Motor Current @V2",{"$f":"B$3 * B14/B$2","v":17.777777777777779},"A"]
["Power 3",{"$f":"B14*B15","v":568.88888888888891},"W"]
[]
["Error Flag Behavior","Value","Units","Description"]
["Vcc",3.3,"v"]
["EF leakage",10,"uA"]
["Nominal equiv R",{"$f":"B19/(B20*0.000001)","v":330000},"ohm"]
["Pullup",{"$f":"Resistor(75000)","v":75000},"ohm"]
["EF V leakage",{"$f":"B19*B21/(B22+B21)","v":2.6888888888888891},"bill25"]
[]
["PIC Input High (TTL)",2,"v"]
["PIC Input High (TTL2)",{"$f":"0.8+0.25*B19","v":1.625},"v"]
["PIC Input High (Schmitt)",{"$f":"0.8*B19","v":2.64},"v"]
["PIC Input High (I2C)",{"$f":"0.7*B19","v":2.3099999999999996},"v"]
["PIC Input High (SMBus)",2.1,"v"]

{"sheet":"Acoustic","index":10,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["Acoustic Signal"]
["4khz - http://www.soundsnap.com/search/audio/4khz/popular"]
["2khz - http://www.soundsnap.com/search/audio/2khz/popular"]
[]
["Manufacturer","Freq","Temp Range","$ ea","$ @500","Web"]
[]
["CUI Inc (smd)","4 khz","'-30 + 70","$4.81 qty 1","$2.49 qty 500","http://search.digikey.com/us/en/products/CMI-1240/102-1196-5-ND/504829"]
["CUI Inc (thru hole)","4 khz","'-20 +70","$3.19 qty 1","$1.65 qty 500","http://search.digikey.com/us/en/products/CEP-2242/102-1115-ND/412374"]
["PUI Audio (thru hole)","4 khz","'-20 +70","$3.66 qty 1","$2.20 qty 500","http://search.digikey.com/us/en/products/AI-1440-TWT-12V-R/668-1024-ND/1464763"]
["Mallory (thru hole)","4.1 khz","'-20 + 90","$2.43 qty 1","$2.09 qty 500","http://search.digikey.com/us/en/products/PK-12N40PQ/458-1066-ND/969793"]
["Kobiton (thru hole)","4 khz","'-20 + 105","$4.26 qty 1","$2.59 qty 500","http://www.mouser.com/ProductDetail/Kobitone/254-15210-ROX/?qs=05UEgX2TgG1gFl%2faATOCEw%3d%3d"]
[]
[]
[]
["Acoustic Supply",12,"v"]
["Acoustic Current",5.0000000000000001E-3,"A"]
["Driver gain (min)",50]
["Base Drive Current",{"$f":"B16/B17","v":1E-4},"A"]
["Base Drive Voltage",3.3,"v"]
["Base Drive Resistance",{"$f":"B19/B18","v":33000}]

{"sheet":"LIN Xcvr","index":11,"n_rows":26,"n_cols":17,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
["Vendor","Part #","LIN V","Price","Qty","V Reg","Vreg","Temp","V Supply","Bus Voltage","Load Dump","3v IO","Normal","Sleep","Standby","Wakup Pin","Tx timeout"]
["ON Semi","NCV7321",null,null,null,"N",null,"-40, +125",27,45,"45v","Y","Y","20 uA","Y"]
["TI","SN65HVDA195-Q1",null,0.47,1000,"N",null,"-40, +125",27,40,null,"Y",null,null,null,"Y","No"]
["TI","TPIC1021A-Q1 -",null,0.4,1000,"N",null,"-40, +125",27,40,null,"Y",null,null,null,"Y","Yes"]
["NXP","TJA1028TK/3V3",null,null,null,"Y","3.3v @ 70mA","-40, +150",40,40,null,"Y",null,"12uA","45uA",null,"Yes"]
["NXP","TJA1028TK/5V0",null,0.7,1500,"Y","5.0v @ 70mA","-40, +150",40,40,null,"Y",null,"12uA","45uA",null,"Yes"]
["NXP","TJA1021",2.1,0.46,2500,"N",null,"-40, +150",40,null,null,null,null,null,null,null,"Yes"]
["NXP","TJA1022",2.2000000000000002,null,null,"N",null,"-40, +150",40,null,null,null,null,null,null,null,"Yes"]
["Infineon","TLE6258",2]
["Infineon","TLE7259-2GE",2]
["Infineon","TLE8458GV33",2.1,1.03,2500,"Y","3.3 @ 50mA",null,null,null,null,"Y","Y",null,null,"Y","Yes"]
["Infineon","TLE8458G",2.1,1.03,2500,"Y","5.0 @ 50mA","-40, +150",40,40,null,"Y",null,null,null,"Y"]
["Micrchip","MCP2021",2.1,0.95,500,"Y","3.3 @ 50mA","-40, +125",30,null,43]
["Micrchip","MCP2021",2.1,0.95,500,"Y","5.0 @ 50mA","-40, +125",30,null,43]
[]
[]
["LIN Master","Value","Units"]
["Vsupply",27,"v"]
["Resistor",1000,"ohm"]
["Power Dis",{"$f":"B18^2/B19","v":0.72899999999999998},"W"]
["Current",{"$f":"B18/B19","v":2.7E-2},"A"]
[]
["Microcontroller",null,null,null,null,"Qtouch"]
["Atmel","ATA66xx",null,2.81,1000]
["Atmel","ATmega16M1",null,3.87,1600]
["Atmel","ATtiny167",null,1.75,1500]

{"sheet":"Ribbon Con","index":12,"n_rows":30,"n_cols":4,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
["Pin","X","Y","Units"]
[1,{"$f":"-2.5-1.25/2","v":-3.125},1,"mm"]
[2,{"$f":"(A3-A$2)*1.25+B$2","v":-1.875},{"$f":"C2-2","v":-1},"mm"]
[3,{"$f":"(A4-A$2)*1.25+B$2","v":-0.625},{"$f":"C2","v":1},"mm"]
[4,{"$f":"(A5-A$2)*1.25+B$2","v":0.625},{"$f":"C3","v":-1},"mm"]
[5,{"$f":"(A6-A$2)*1.25+B$2","v":1.875},{"$f":"C4","v":1},"mm"]
[6,{"$f":"(A7-A$2)*1.25+B$2","v":3.125},{"$f":"C5","v":-1},"mm"]
[]
["Housing Left",{"$f":"-13.25/2","v":-6.625}]
["Housing Right",{"$f":"-B9","v":6.625}]
["Slot Left",{"$f":"-8.95/2","v":-4.4749999999999996}]
["Slot Right",{"$f":"-B11","v":4.4749999999999996}]
[]
[]
[]
["Pin","X","Y","Units"]
[1,-1.25,1,"mm"]
[2,{"$f":"(A18-A$17)*1.25+B$17","v":0},{"$f":"C17-2","v":-1},"mm"]
[3,{"$f":"(A19-A$17)*1.25+B$17","v":1.25},{"$f":"C17","v":1},"mm"]
[]
[]
["Housing Left",{"$f":"-9.5/2","v":-4.75}]
["Housing Right",{"$f":"-B22","v":4.75}]
["Slot Left",{"$f":"-5.2/2","v":-2.6}]
["Slot Right",{"$f":"-B24","v":2.6}]
[]
[null,84.86,"mm"]
[null,{"$f":"B27/25.4","v":3.3409448818897638}]
[null,21.79,"mm"]
[null,{"$f":"B29/25.4","v":0.85787401574803146}]

{"sheet":"Block Cost","index":13,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Functional Block","Est. Cost","Qty",null,"Notes"]
["Micro",4.5,2000,null,"micro, crystal, caps"]
["Config Storage",0.25,2000,null,"eerom"]
["Power Supply",4,2000,null,"switching"]
["Learn Mode",0.1,2000,null,"2xR, 1xC"]
["Wakeup In",0.25,2000]
["Wakeup Out",1,2000]
["LIN Transceiver",1,2000]
["CAN Transceiver",1,2000,null,"xcvr, filter, diodes"]
["H-Driver",3.75,2000]
["LED Driver",0.1,2000]
["Keypad Sense",0.25,2000]
["Acoustic Signal",2.25,2000,null,"need to find -40 to +85 part"]
["Miscellaneous",3,2000,null,"whatever was forgotton above"]
["Estimated Total",{"$f":"SUM(B2:B14)","v":21.45}]
[]
[]
[]
["Estimated costs includes the primary and supporting components"]
[]
[]
[]
[]
[null,"LIN","CAN","JD Exclusive","Description"]
[null,"Yes","No","No","smaller micro, no JD/OS"]
[null,"No","Yes","Yes","JD/OS, \"fully integrated\""]
[null,"No","Yes","No","powerful micro, ~25-50,000 lines of code"]

{"sheet":"Components","index":14,"n_rows":46,"n_cols":4,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
["Category","ScratchNotes","Additional Notes"]
["H-Bridge","BTN7960/70/71","half-Bridge 40V 40A","requires 2 part"]
["H-Bridge","TLE6208-3","3 half-bridge .8A 32v","0.8A not enough"]
["H-Bridge","TLE8201R","Full Door module - Mirror w/heat/light","too many functions - cost"]
["H-Bridge","TLE8203E","Full Door module - Mirror w/heat/light","not enough current"]
["H-Bridge","TLE84106EL","Hex half-bridge","18v, 0.8A"]
["H-Bridge","TLE7181EM","H-Bridge Driver: 34v, 10 uA quiescient, lots of features (may cost too much)","Pre-Driver for mosfets"]
["H-Bridge","BTM7740G","8A peak (25C), 5uA quiesc, 40V"]
["H-Bridge","TLE5205","4A 40V status"]
["H-Bridge","TLE5206","4A 40V status"]
[]
[null,"BTS50015","Single high-side 28V 33A, 18uA standby","If we need a pre-enable"]
[]
["System Basis Chip","TLE8261E","System Basis Chip, reg, CAN transceiver, watchdog","very interesting combination of parts, but for a system that does not need them all, this is overkill and no alternate sourcing."]
["System Basis Chip","TLE8262E","1xLIN"]
["System Basis Chip","TLE8263E","2xLIN"]
["System Basis Chip","TLE8264E","3xLIN"]
["System Basis Chip","TLE6266G","CAN, Watchdog","on special request only"]
["Window Lift Module","TLE7810","Full Window Control on LIN w/8051"]
[]
[]
["Power Supply","TLE6365G","step down w/reset 8 to 40v","no enable"]
["Power Supply","TLE6711G","boost/buck, watchdog, enable","watchdog compatibility"]
["Power Supply","TLE7368E","5.5v, reset, watchdog","overkill - for high end multi-voltage"]
["Power Supply","TLE4278G","Reset, watchdog","linear part, but with possibly adequate heat-sink"]
["Power Supply","LTC3115-1","buck-boost, 2.7-40v, 5v1A out, enable, burst mode"]
["Power Supply","LT3433","buck-boost, 4-60v, 5v .3A, enable"]
["Power Supply","LT3689","step-down, por, wdt","wdt compatibility?"]
["Power Supply","LT3682","uPower step down,"]
["Power Supply","LT3631","4.5 to 45 to 5v@100mA","nice, but 100mA max"]
["Power Supply","LT3470A","buck reg 12v to 5v@250mA","8-pin"]
["Power Supply","LTM8021","7.5-36v to 5v@500mA","full uModule w most parts (LGA pkg)"]
["Power Supply","LT3502","7-40v to 5v@500mA"]
["Power Supply","LT3970","7-40 to 5v@350mA, enable, power good out","10-pin"]
["Power Supply","LT1934ES6","6.5-34v to 5v@250mA, enable","6-pin"]
[]
[]
[]
["Capacitive Touch Sense",null,"Can share matrix with backlight LEDs"]
[]
[]
["Key","Not yet analyzed","part identified from initial scan/research"]
[null,"Candidate Parts","looks even better"]
[null,"Candidate Parts","seems to mee the requirements"]
[null,"Defer rejection","further analysis may be required"]
[null,"Rejected","not appropriate for this project (reason noted)"]