{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Activities","Power Supply"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Activities","index":0,"n_rows":16,"n_cols":2,"rows_kept":16,"flags":["formulas_cached_only"]}
["Block","Activity Description"]
["Micro","Vcc"]
["Micro","Oscillator"]
["Micro","Pin configurations"]
["Micro","Current Source"]
["Micro","Current Sink"]
["Micro","CAN"]
["Micro","LED Drive"]
["Micro","Keypad Sense"]
["Micro","Acoustic Signal"]
["Micro","LIN"]
["Micro","Wakeup Out"]
["Micro","Wakeup In"]
["Micro","H-Bridge"]
["Power Supply"]
["H-Bridge"]

{"sheet":"Power Supply","index":1,"n_rows":3,"n_cols":3,"rows_kept":3,"flags":["formulas_cached_only"]}
["Part Number","Supplier","Description"]
["TDA3673AT","NXP","45v in 3.3v out 100 mA, with active high Enable, Ven input max 18v"]
["TDA3664AT","NXP","45v in 5.0v out 100 mA"]