{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Tracking","HW Activities","Power Supply Notes"],"not_rendered":{"external_links":2,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tracking","index":0,"n_rows":69,"n_cols":7,"rows_kept":69,"flags":["formulas_cached_only"]}
["Issue ID","State","Assigned to","Description","Last Update","Next Update","Close Notes"]
[{"v":1,"d":"001"},"Review","Dave S","Micro Selection - determine JD/OS compatibility","2011-12-23","2012-01-03","XC2224L appears to be JD/OS compatible"]
[{"v":2,"d":"002"},"New","Dave S","Acquire two XC2224L Evaluation Kits (Bob, Dave S)","2011-12-23"]
[{"v":3,"d":"003"},"Assigned","Dave M","Acquire JD/OS User license","2011-12-23"]
[{"v":4,"d":"004"},"New","Dave S","Develop electrical characteristic proposal for C&F","2011-12-23"]
[{"v":5,"d":"005"},"New","Dave M","FTP Site Configuration","2011-12-23","2012-01-10"]
[{"v":6,"d":"006"},"New",null,"Configuration Management Server - C&F StarTeam?","2011-12-23"]
[{"v":7,"d":"007"},"Assigned","Dave M","Keypad backlight - EL or LED","2011-12-23"]
[{"v":8,"d":"008"},"New","C&F","Provide CAN message spreadsheet (auto-generates code)","2011-12-23","2012-02-01"]
[{"v":9,"d":"009"},"New","C&F","Provide Diagnostic Address List and functions","2011-12-23","2012-02-01"]
[{"v":10,"d":"010"},"Assigned","Dave S","H-Bridge research","2011-12-23","2012-01-03"]
[{"v":11,"d":"011"},"Assigned","Dave S","Acoustic signal research (size matters)","2011-12-23","2012-01-03"]
[{"v":12,"d":"012"},"New","Bob L","Emulate EEPROM in Flash to eliminate external chip","2011-12-23","2012-01-10","saves precious board space and cost"]
[{"v":13,"d":"013"},"New","Dave S","Review Errata sheet","2011-12-23","2012-01-10"]
[{"v":14,"d":"014"},"New","Bob L","Review Errata sheet","2011-12-23","2012-01-10"]
[{"v":15,"d":"015"},"New","Bob L","LIN Slave Driver - any special pinout","2011-12-23","2012-02-10"]
[{"v":16,"d":"016"},"New","Dave M","Desktop Screen Sharing Tool","2011-12-23","2012-01-03"]
[{"v":17,"d":"017"},"New","Dave S","Automated Testing tool and practices","2011-12-23","2012-01-03"]
[{"v":18,"d":"018"},"New","Dave M","\"SW Owned by…\" related to the \"business logic we create\"","2011-12-23","2012-01-10","Need to know before we put SW anywhere"]
[{"v":19,"d":"019"},"New","Dave M","Requirements document - initial creation","2011-12-23","2012-01-03"]
[{"v":20,"d":"020"}]
[{"v":21,"d":"021"}]
[{"v":22,"d":"022"}]
[{"v":23,"d":"023"}]
[{"v":24,"d":"024"}]
[{"v":25,"d":"025"}]
[{"v":26,"d":"026"}]
[{"v":27,"d":"027"}]
[{"v":28,"d":"028"}]
[{"v":29,"d":"029"}]
[{"v":30,"d":"030"}]
[{"v":31,"d":"031"}]
[{"v":32,"d":"032"}]
[{"v":33,"d":"033"}]
[{"v":34,"d":"034"}]
[{"v":35,"d":"035"}]
[{"v":36,"d":"036"}]
[{"v":37,"d":"037"}]
[{"v":38,"d":"038"}]
[{"v":39,"d":"039"}]
[{"v":40,"d":"040"}]
[{"v":41,"d":"041"}]
[{"v":42,"d":"042"}]
[{"v":43,"d":"043"}]
[{"v":44,"d":"044"}]
[{"v":45,"d":"045"}]
[{"v":46,"d":"046"}]
[{"v":47,"d":"047"}]
[{"v":48,"d":"048"}]
[{"v":49,"d":"049"}]
[{"v":50,"d":"050"}]
[{"v":51,"d":"051"}]
[{"v":52,"d":"052"}]
[{"v":53,"d":"053"}]
[{"v":54,"d":"054"}]
[{"v":55,"d":"055"}]
[{"v":56,"d":"056"}]
[{"v":57,"d":"057"}]
[{"v":58,"d":"058"}]
[{"v":59,"d":"059"}]
[{"v":60,"d":"060"}]
[{"v":61,"d":"061"},null,null,"Copy this row to make another with the formats"]
[]
[null,"States","Resources"]
[null,"New","Dave M"]
[null,"Assigned","Dave S"]
[null,"Review","Bob L"]
[null,"Closed","C&F"]
[null,null,"Other"]

{"sheet":"HW Activities","index":1,"n_rows":16,"n_cols":3,"rows_kept":16,"flags":["formulas_cached_only"]}
["Block","Activity Description"]
["Micro","Vcc"]
["Micro","Oscillator"]
["Micro","Pin configurations"]
["Micro","Current Source"]
["Micro","Current Sink"]
["Micro","CAN"]
["Micro","LED Drive"]
["Micro","Keypad Sense"]
["Micro","Acoustic Signal"]
["Micro","LIN","Infineon LIN Slave for XC"]
["Micro","Wakeup Out"]
["Micro","Wakeup In"]
["Micro","H-Bridge"]
["Power Supply"]
["H-Bridge"]

{"sheet":"Power Supply Notes","index":2,"n_rows":3,"n_cols":3,"rows_kept":3,"flags":["formulas_cached_only"]}
["Part Number","Supplier","Description"]
["TDA3673AT","NXP","45v in 3.3v out 100 mA, with active high Enable, Ven input max 18v"]
["TDA3664AT","NXP","45v in 5.0v out 100 mA"]