{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["Volume Level","Commands","Sheet1","System Status","Status Block"],"not_rendered":{"charts":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Volume Level","index":0,"n_rows":234,"n_cols":8,"rows_kept":234}
[null,null,"Dec","Hex","Documented db","Onscreen db"]
[null,null,232,{"$f":"DEC2HEX(C2,2)","v":"E8"},16.5]
[null,null,231,{"$f":"DEC2HEX(C3,2)","v":"E7"},{"$f":"(C3-$C$35)/($C$2-$C$35)*($E$2-$E$35)","v":{"v":16,"d":"16.0"}}]
[null,null,230,"E6",{"$f":"(C4-$C$35)/($C$2-$C$35)*($E$2-$E$35)","v":15.5}]
[null,null,229,"E5",{"v":15,"d":"15.0"}]
[null,null,228,"E4",14.5]
[null,null,227,"E3",{"v":14,"d":"14.0"}]
[null,null,226,"E2",13.5]
[null,null,225,"E1",{"v":13,"d":"13.0"}]
[null,null,224,"E0",12.5]
[null,null,223,"DF",{"v":12,"d":"12.0"}]
[null,null,222,"DE",11.5]
[null,null,221,"DD",{"v":11,"d":"11.0"}]
[null,null,220,"DC",10.5]
[null,null,219,"DB",{"v":10,"d":"10.0"}]
[null,null,218,"DA",9.5]
[null,null,217,"D9",{"v":9,"d":"9.0"}]
[null,null,216,"D8",8.5]
[null,null,215,"D7",{"v":8,"d":"8.0"}]
[null,null,214,"D6",7.5]
[null,null,213,"D5",{"v":7,"d":"7.0"}]
[null,null,212,"D4",6.5]
[null,null,211,"D3",{"v":6,"d":"6.0"}]
[null,null,210,"D2",5.5]
[null,null,209,"D1",{"v":5,"d":"5.0"}]
[null,null,208,"D0",4.5]
[null,null,207,"CF",{"v":4,"d":"4.0"}]
[null,null,206,"CE",3.5]
[null,null,205,"CD",{"v":3,"d":"3.0"}]
[null,null,204,"CC",2.5]
[null,null,203,"CB",{"v":2,"d":"2.0"}]
[null,null,202,"CA",1.5]
[null,null,201,"C9",{"v":1,"d":"1.0"}]
[null,null,200,"C8",0.5]
[null,null,199,"C7",{"v":0,"d":"0.0"}]
[null,null,198,"C6",-0.5]
[null,null,197,"C5",{"$f":"(C37-$C$35)/($C$177-$C$35)*($E$177-$E$35)","v":{"v":-1.1267605633802817,"d":"-1.1"}}]
[null,null,196,"C4",{"v":-1.6901408450704225,"d":"-1.7"}]
[null,null,195,"C3",{"v":-2.2535211267605635,"d":"-2.3"}]
[null,null,194,"C2",{"v":-2.8169014084507045,"d":"-2.8"}]
[null,null,193,"C1",{"v":-3.380281690140845,"d":"-3.4"}]
[null,null,192,"C0",{"v":-3.9436619718309855,"d":"-3.9"}]
[null,null,191,"BF",{"v":-4.507042253521127,"d":"-4.5"}]
[null,null,190,"BE",{"v":-5.070422535211268,"d":"-5.1"}]
[null,null,189,"BD",{"v":-5.633802816901409,"d":"-5.6"}]
[null,null,188,"BC",{"v":-6.197183098591549,"d":"-6.2"}]
[null,null,187,"BB",{"v":-6.76056338028169,"d":"-6.8"}]
[null,null,186,"BA",{"v":-7.323943661971831,"d":"-7.3"}]
[null,null,185,"B9",{"v":-7.887323943661971,"d":"-7.9"}]
[null,null,184,"B8",{"v":-8.450704225352112,"d":"-8.5"}]
[null,null,183,"B7",{"v":-9.014084507042254,"d":"-9.0"}]
[null,null,182,"B6",{"v":-9.577464788732394,"d":"-9.6"}]
[null,null,181,"B5",{"v":-10.140845070422536,"d":"-10.1"}]
[null,null,180,"B4",{"v":-10.704225352112676,"d":"-10.7"}]
[null,null,179,"B3",{"v":-11.267605633802818,"d":"-11.3"}]
[null,null,178,"B2",{"v":-11.830985915492958,"d":"-11.8"}]
[null,null,177,"B1",{"v":-12.394366197183098,"d":"-12.4"}]
[null,null,176,"B0",{"v":-12.95774647887324,"d":"-13.0"}]
[null,null,175,"AF",{"v":-13.52112676056338,"d":"-13.5"},{"v":-12,"d":"-12.0"},{"$f":"(C59-C75)","v":16},{"$f":"ABS(E75-E59)","v":9.014084507042256}]
[null,null,174,"AE",{"v":-14.08450704225352,"d":"-14.1"}]
[null,null,173,"AD",{"v":-14.647887323943662,"d":"-14.6"}]
[null,null,172,"AC",{"v":-15.211267605633802,"d":"-15.2"}]
[null,null,171,"AB",{"v":-15.774647887323942,"d":"-15.8"}]
[null,null,170,"AA",{"v":-16.338028169014084,"d":"-16.3"}]
[null,null,169,"A9",{"v":-16.901408450704224,"d":"-16.9"}]
[null,null,168,"A8",{"v":-17.464788732394364,"d":"-17.5"}]
[null,null,167,{"$f":"DEC2HEX(C67,2)","v":"A7"},{"v":-18.028169014084508,"d":"-18.0"}]
[null,null,166,"A6",{"v":-18.591549295774648,"d":"-18.6"}]
[null,null,165,"A5",{"v":-19.154929577464788,"d":"-19.2"}]
[null,null,164,"A4",{"v":-19.718309859154928,"d":"-19.7"}]
[null,null,163,"A3",{"v":-20.281690140845072,"d":"-20.3"}]
[null,null,162,"A2",{"v":-20.84507042253521,"d":"-20.8"}]
[null,null,161,"A1",{"v":-21.408450704225352,"d":"-21.4"}]
[null,null,160,"A0",{"v":-21.971830985915496,"d":"-22.0"}]
[null,null,159,"9F",{"v":-22.535211267605636,"d":"-22.5"},{"v":-20,"d":"-20.0"}]
[null,null,158,"9E",{"v":-23.098591549295776,"d":"-23.1"}]
[null,null,157,"9D",{"v":-23.661971830985916,"d":"-23.7"}]
[null,null,156,"9C",{"v":-24.225352112676056,"d":"-24.2"}]
[null,null,155,"9B",{"v":-24.788732394366196,"d":"-24.8"}]
[null,null,154,"9A",{"v":-25.35211267605634,"d":"-25.4"}]
[null,null,153,"99",{"v":-25.91549295774648,"d":"-25.9"}]
[null,null,152,"98",{"v":-26.47887323943662,"d":"-26.5"}]
[null,null,151,"97",{"v":-27.04225352112676,"d":"-27.0"}]
[null,null,150,"96",{"v":-27.6056338028169,"d":"-27.6"}]
[null,null,149,"95",{"v":-28.16901408450704,"d":"-28.2"}]
[null,null,148,"94",{"v":-28.732394366197184,"d":"-28.7"}]
[null,null,147,"93",{"v":-29.295774647887324,"d":"-29.3"}]
[null,null,146,"92",{"v":-29.859154929577464,"d":"-29.9"}]
[null,null,145,"91",{"v":-30.422535211267604,"d":"-30.4"}]
[null,null,144,"90",{"v":-30.985915492957744,"d":"-31.0"}]
[null,null,143,"8F",{"v":-31.549295774647884,"d":"-31.5"}]
[null,null,142,"8E",{"v":-32.11267605633803,"d":"-32.1"}]
[null,null,141,"8D",{"v":-32.67605633802817,"d":"-32.7"}]
[null,null,140,"8C",{"v":-33.23943661971831,"d":"-33.2"}]
[null,null,139,"8B",{"v":-33.80281690140845,"d":"-33.8"}]
[null,null,138,"8A",{"v":-34.36619718309859,"d":"-34.4"}]
[null,null,137,"89",{"v":-34.92957746478873,"d":"-34.9"}]
[null,null,136,"88",{"v":-35.49295774647887,"d":"-35.5"}]
[null,null,135,"87",{"v":-36.056338028169016,"d":"-36.1"}]
[null,null,134,"86",{"v":-36.61971830985915,"d":"-36.6"}]
[null,null,133,"85",{"$f":"(C101-$C$35)/($C$177-$C$35)*($E$177-$E$35)","v":{"v":-37.183098591549296,"d":"-37.2"}}]
[null,null,132,"84",{"v":-37.74647887323943,"d":"-37.7"}]
[null,null,131,"83",{"v":-38.309859154929576,"d":"-38.3"}]
[null,null,130,"82",{"v":-38.87323943661972,"d":"-38.9"}]
[null,null,129,"81",{"v":-39.436619718309856,"d":"-39.4"}]
[null,null,128,"80",{"v":-40,"d":"-40.0"}]
[null,null,127,"7F",{"v":-40.563380281690144,"d":"-40.6"}]
[null,null,126,"7E",{"v":-41.12676056338028,"d":"-41.1"}]
[null,null,125,"7D",{"v":-41.69014084507042,"d":"-41.7"}]
[null,null,124,"7C",{"v":-42.25352112676056,"d":"-42.3"}]
[null,null,123,"7B",{"v":-42.816901408450704,"d":"-42.8"}]
[null,null,122,"7A",{"v":-43.38028169014085,"d":"-43.4"}]
[null,null,121,"79",{"v":-43.94366197183099,"d":"-43.9"}]
[null,null,120,"78",{"v":-44.50704225352113,"d":"-44.5"}]
[null,null,119,"77",{"v":-45.07042253521127,"d":"-45.1"},{"v":-40,"d":"-40.0"}]
[null,null,118,"76",{"v":-45.63380281690141,"d":"-45.6"}]
[null,null,117,"75",{"v":-46.19718309859155,"d":"-46.2"}]
[null,null,116,"74",{"v":-46.76056338028169,"d":"-46.8"}]
[null,null,115,"73",{"v":-47.32394366197183,"d":"-47.3"}]
[null,null,114,"72",{"v":-47.88732394366197,"d":"-47.9"}]
[null,null,113,"71",{"v":-48.45070422535211,"d":"-48.5"}]
[null,null,112,"70",{"v":-49.01408450704225,"d":"-49.0"}]
[null,null,111,"6F",{"v":-49.57746478873239,"d":"-49.6"}]
[null,null,110,"6E",{"v":-50.14084507042254,"d":"-50.1"}]
[null,null,109,"6D",{"v":-50.70422535211268,"d":"-50.7"}]
[null,null,108,"6C",{"v":-51.267605633802816,"d":"-51.3"}]
[null,null,107,"6B",{"v":-51.83098591549296,"d":"-51.8"}]
[null,null,106,"6A",{"v":-52.3943661971831,"d":"-52.4"}]
[null,null,105,"69",{"v":-52.95774647887324,"d":"-53.0"}]
[null,null,104,"68",{"v":-53.52112676056338,"d":"-53.5"}]
[null,null,103,{"$f":"DEC2HEX(C131,2)","v":"67"},{"v":-54.08450704225352,"d":"-54.1"}]
[null,null,102,"66",{"v":-54.647887323943664,"d":"-54.6"}]
[null,null,101,"65",{"v":-55.2112676056338,"d":"-55.2"}]
[null,null,100,"64",{"v":-55.77464788732394,"d":"-55.8"}]
[null,null,99,"63",{"v":-56.33802816901408,"d":"-56.3"},{"v":-50,"d":"-50.0"}]
[null,null,98,"62",{"v":-56.90140845070423,"d":"-56.9"}]
[null,null,97,"61",{"v":-57.46478873239437,"d":"-57.5"}]
[null,null,96,"60",{"v":-58.02816901408451,"d":"-58.0"}]
[null,null,95,"5F",{"v":-58.59154929577465,"d":"-58.6"}]
[null,null,94,"5E",{"v":-59.15492957746479,"d":"-59.2"}]
[null,null,93,"5D",{"v":-59.71830985915493,"d":"-59.7"}]
[null,null,92,"5C",{"v":-60.28169014084507,"d":"-60.3"}]
[null,null,91,"5B",{"v":-60.84507042253521,"d":"-60.8"}]
[null,null,90,"5A",{"v":-61.40845070422535,"d":"-61.4"}]
[null,null,89,"59",{"v":-61.97183098591549,"d":"-62.0"}]
[null,null,88,"58",{"v":-62.53521126760563,"d":"-62.5"}]
[null,null,87,"57",{"v":-63.09859154929577,"d":"-63.1"}]
[null,null,86,"56",{"v":-63.66197183098592,"d":"-63.7"}]
[null,null,85,"55",{"v":-64.22535211267606,"d":"-64.2"}]
[null,null,84,"54",{"v":-64.7887323943662,"d":"-64.8"}]
[null,null,83,"53",{"v":-65.35211267605634,"d":"-65.4"}]
[null,null,82,"52",{"v":-65.91549295774648,"d":"-65.9"}]
[null,null,81,"51",{"v":-66.47887323943662,"d":"-66.5"}]
[null,null,80,"50",{"v":-67.04225352112675,"d":"-67.0"}]
[null,null,79,"4F",{"v":-67.6056338028169,"d":"-67.6"}]
[null,null,78,"4E",{"v":-68.16901408450704,"d":"-68.2"}]
[null,null,77,"4D",{"v":-68.73239436619718,"d":"-68.7"}]
[null,null,76,"4C",{"v":-69.29577464788733,"d":"-69.3"}]
[null,null,75,"4B",{"v":-69.85915492957746,"d":"-69.9"}]
[null,null,74,"4A",{"v":-70.42253521126761,"d":"-70.4"}]
[null,null,73,"49",{"v":-70.98591549295774,"d":"-71.0"}]
[null,null,72,"48",{"v":-71.54929577464789,"d":"-71.5"}]
[null,null,71,"47",{"v":-72.11267605633803,"d":"-72.1"}]
[null,null,70,"46",{"v":-72.67605633802818,"d":"-72.7"}]
[null,null,69,"45",{"$f":"(C165-$C$35)/($C$177-$C$35)*($E$177-$E$35)","v":{"v":-73.2394366197183,"d":"-73.2"}}]
[null,null,68,"44",{"v":-73.80281690140845,"d":"-73.8"}]
[null,null,67,"43",{"v":-74.36619718309859,"d":"-74.4"}]
[null,null,66,"42",{"v":-74.92957746478874,"d":"-74.9"}]
[null,null,65,"41",{"v":-75.49295774647887,"d":"-75.5"}]
[null,null,64,"40",{"v":-76.05633802816901,"d":"-76.1"}]
[null,null,63,"3F",{"v":-76.61971830985915,"d":"-76.6"}]
[null,null,62,"3E",{"v":-77.1830985915493,"d":"-77.2"}]
[null,null,61,"3D",{"v":-77.74647887323944,"d":"-77.7"}]
[null,null,60,"3C",{"v":-78.30985915492958,"d":"-78.3"}]
[null,null,59,"3B",{"v":-78.87323943661971,"d":"-78.9"}]
[null,null,58,"3A",{"v":-79.43661971830986,"d":"-79.4"}]
[null,null,57,"39",{"v":-80,"d":"-80.0"}]
[null,null,56,"38"]
[null,null,55,"37"]
[null,null,54,"36"]
[null,null,53,"35"]
[null,null,52,"34"]
[null,null,51,"33"]
[null,null,50,"32"]
[null,null,49,"31"]
[null,null,48,"30"]
[null,null,47,"2F"]
[null,null,46,"2E"]
[null,null,45,"2D"]
[null,null,44,"2C"]
[null,null,43,"2B"]
[null,null,42,"2A"]
[null,null,41,"29"]
[null,null,40,"28"]
[null,null,39,{"$f":"DEC2HEX(C195,2)","v":"27"},null,{"v":-80,"d":"-80.0"}]
[null,null,38,"26"]
[null,null,37,"25"]
[null,null,36,"24"]
[null,null,35,"23"]
[null,null,34,"22"]
[null,null,33,"21"]
[null,null,32,"20"]
[null,null,31,"1F"]
[null,null,30,"1E"]
[null,null,29,"1D"]
[null,null,28,"1C"]
[null,null,27,"1B"]
[null,null,26,"1A"]
[null,null,25,"19"]
[null,null,24,"18"]
[null,null,23,"17"]
[null,null,22,"16"]
[null,null,21,"15"]
[null,null,20,"14"]
[null,null,19,"13"]
[null,null,18,"12"]
[null,null,17,"11"]
[null,null,16,"10"]
[null,null,15,"0F"]
[null,null,14,"0E"]
[null,null,13,"0D"]
[null,null,12,"0C"]
[null,null,11,"0B"]
[null,null,10,"0A"]
[null,null,9,"09"]
[null,null,8,"08"]
[null,null,7,"07"]
[null,null,6,"06"]
[null,null,5,"05"]
[null,null,4,"04"]
[null,null,3,"03"]
[null,null,2,"02"]
[null,null,1,"01"]
[null,null,0,"00"]

{"sheet":"Commands","index":1,"n_rows":220,"n_cols":20,"rows_kept":220}
["SW","CMDT0","CMDT1","CMDT2","CMDT3","function","setting","Type","RCMD1,2","Subsystem","Function",null,"Prefix","Msg","Suffix",null,"sub","Func","Arg","Msg"]
[0,7,"A",1,"A","master volume","Up",0,26,"subMain","fncVolume","eUp","\\x02",{"$f":"A2&B2&C2&D2&E2","v":"07A1A"},"\\x03",null,{"$f":"\"AVRSubsys::\" & J2","v":"AVRSubsys::subMain"},{"$f":"\"AVRFunc::\" & K2","v":"AVRFunc::fncVolume"},{"$f":"\"AVRInterface::\"&L2","v":"AVRInterface::eUp"},{"$f":"M2&N2&O2","v":"\\x0207A1A\\x03"}]
[0,7,"A",1,"B",null,"Down    ",null,null,"subMain","fncVolume","eDown","\\x02",{"$f":"A3&B3&C3&D3&E3","v":"07A1B"},"\\x03",null,{"$f":"\"AVRSubsys::\" & J3","v":"AVRSubsys::subMain"},{"$f":"\"AVRFunc::\" & K3","v":"AVRFunc::fncVolume"},{"$f":"\"AVRInterface::\"&L3","v":"AVRInterface::eDown"},{"$f":"M3&N3&O3","v":"\\x0207A1B\\x03"}]
[0,7,"E","A",2,"Audio Mute","ON",null,23,"subMain","fncMute","eOn","\\x02","07EA2","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncMute","AVRInterface::eOn","\\x0207EA2\\x03"]
[0,7,"E","A",3,null,"OFF    ",null,null,"subMain","fncMute","eOff","\\x02","07EA3","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncMute","AVRInterface::eOff","\\x0207EA3\\x03"]
[0,7,"A",1,4,"Input  ","PHONO",null,21,"subMain","fncInput","ePhono","\\x02","07A14","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::ePhono","\\x0207A14\\x03"]
[0,7,"A",1,5,null,"CD    ",null,null,"subMain","fncInput","eCD","\\x02","07A15","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eCD","\\x0207A15\\x03"]
[0,7,"A",1,6,null,"TUNER    ",null,null,"subMain","fncInput","eTuner","\\x02","07A16","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eTuner","\\x0207A16\\x03"]
[0,7,"A",1,9,null,"CD-R    ",null,null,"subMain","fncInput","eCDR","\\x02","07A19","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eCDR","\\x0207A19\\x03"]
[0,7,"A","C",9,null,"MD/TAPE    ",null,null,"subMain","fncInput","eMD_Tape","\\x02","07AC9","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eMD_Tape","\\x0207AC9\\x03"]
[0,7,"A","C",1,null,"DVD    ",null,null,"subMain","fncInput","eDVD","\\x02","07AC1","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eDVD","\\x0207AC1\\x03"]
[0,7,"A",5,4,null,"D-TV/LD    ",null,null,"subMain","fncInput","eDTV","\\x02","07A54","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eDTV","\\x0207A54\\x03"]
[0,7,"A","C",0,null,"CABLE ( CBL/SAT ) ",null,null,"subMain","fncInput","eCable","\\x02","07AC0","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eCable","\\x0207AC0\\x03"]
[0,7,"A","C","A",null,"SAT    ",null,null,"subMain","fncInput","eSat","\\x02","07ACA","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eSat","\\x0207ACA\\x03"]
[0,7,"A",0,"F",null,"VCR1    ",null,null,"subMain","fncInput","eVCR1","\\x02","07A0F","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eVCR1","\\x0207A0F\\x03"]
[0,7,"A",1,3,null,"VCR2/DVR    ",null,null,"subMain","fncInput","eVCR2_DVR","\\x02","07A13","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eVCR2_DVR","\\x0207A13\\x03"]
[0,7,"A","C",8,null,"VCR3    ",null,null,"subMain","fncInput","eVCR3","\\x02","07AC8","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eVCR3","\\x0207AC8\\x03"]
[0,7,"A",5,5,null,"V-AUX    ",null,null,"subMain","fncInput","eV_Aux","\\x02","07A55","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInput","AVRInterface::eV_Aux","\\x0207A55\\x03"]
[0,7,"E","A",4,"6ch input","ON",null,null,"subMain","fnc6ChInput","eOn","\\x02","07EA4","\\x03",null,"AVRSubsys::subMain","AVRFunc::fnc6ChInput","AVRInterface::eOn","\\x0207EA4\\x03"]
[0,7,"E","A",5,null,"OFF    ",null,null,"subMain","fnc6ChInput","eOff","\\x02","07EA5","\\x03",null,"AVRSubsys::subMain","AVRFunc::fnc6ChInput","AVRInterface::eOff","\\x0207EA5\\x03"]
[0,7,"E","A",6,"Input Mode ","AUTO",null,22,"subMain","fncInputMode","eAuto","\\x02","07EA6","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInputMode","AVRInterface::eAuto","\\x0207EA6\\x03"]
[0,7,"E","A",7,null,"D.D., RF   ",null,null,"subMain","fncInputMode","eDD_RF","\\x02","07EA7","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInputMode","AVRInterface::eDD_RF","\\x0207EA7\\x03"]
[0,7,"E","A",8,null,"DTS    ",null,null,"subMain","fncInputMode","eDTS","\\x02","07EA8","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInputMode","AVRInterface::eDTS","\\x0207EA8\\x03"]
[0,7,"E","A",9,null,"DIGITAL    ",null,null,"subMain","fncInputMode","eDigital","\\x02","07EA9","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInputMode","AVRInterface::eDigital","\\x0207EA9\\x03"]
[0,7,"E","A","A",null,"ANALOG    ",null,null,"subMain","fncInputMode","eAnalog","\\x02","07EAA","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInputMode","AVRInterface::eAnalog","\\x0207EAA\\x03"]
[0,7,"E",3,"B",null,"AAC    ",null,null,"subMain","fncInputMode","eAAC","\\x02","07E3B","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncInputMode","AVRInterface::eAAC","\\x0207E3B\\x03"]
[0,7,"A","D","A","Zone 2 Volume ","UP",null,27,"subZone2","fncVolume","eUp","\\x02","07ADA","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolume","AVRInterface::eUp","\\x0207ADA\\x03"]
[0,7,"A","D","B",null,"DOWN    ",null,null,"subZone2","fncVolume","eDown","\\x02","07ADB","\\x03",null,{"$f":"\"AVRSubsys::\" & J28","v":"AVRSubsys::subZone2"},{"$f":"\"AVRFunc::\" & K28","v":"AVRFunc::fncVolume"},"AVRInterface::eDown","\\x0207ADB\\x03"]
[0,7,"E","A",0,"Zone2 mute","ON",null,25,"subZone2","fncMute","eOn","\\x02","07EA0","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncMute","AVRInterface::eOn","\\x0207EA0\\x03"]
[0,7,"E","A",1,null,"OFF    ",null,null,"subZone2","fncMute","eOff","\\x02","07EA1","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncMute","AVRInterface::eOff","\\x0207EA1\\x03"]
[0,7,"A","D",0,"Zone2 Input","PHONO",null,24,"subZone2","fncInput","ePhono","\\x02","07AD0","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::ePhono","\\x0207AD0\\x03"]
[0,7,"A","D",1,null,"CD    ",null,null,"subZone2","fncInput","eCD","\\x02","07AD1","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eCD","\\x0207AD1\\x03"]
[0,7,"A","D",2,null,"TUNER    ",null,null,"subZone2","fncInput","eTuner","\\x02","07AD2","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eTuner","\\x0207AD2\\x03"]
[0,7,"A","D",4,null,"CD-R    ",null,null,"subZone2","fncInput","eCDR","\\x02","07AD4","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eCDR","\\x0207AD4\\x03"]
[0,7,"A","C","F",null,"MD/TAPE    ",null,null,"subZone2","fncInput","eMD_Tape","\\x02","07ACF","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eMD_Tape","\\x0207ACF\\x03"]
[0,7,"A","C","D",null,"DVD    ",null,null,"subZone2","fncInput","eDVD","\\x02","07ACD","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eDVD","\\x0207ACD\\x03"]
[0,7,"A","D",9,null,"D-TV/LD    ",null,null,"subZone2","fncInput","eDTV","\\x02","07AD9","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eDTV","\\x0207AD9\\x03"]
[0,7,"A","C","C",null,"CABLE ( CBL/SAT ) ",null,null,"subZone2","fncInput","eCable","\\x02","07ACC","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eCable","\\x0207ACC\\x03"]
[0,7,"A","C","B",null,"SAT    ",null,null,"subZone2","fncInput","eSat","\\x02","07ACB","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eSat","\\x0207ACB\\x03"]
[0,7,"A","D",6,null,"VCR1    ",null,null,"subZone2","fncInput","eVCR1","\\x02","07AD6","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eVCR1","\\x0207AD6\\x03"]
[0,7,"A","D",7,null,"VCR2/DVR    ",null,null,"subZone2","fncInput","eVCR2_DVR","\\x02","07AD7","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eVCR2_DVR","\\x0207AD7\\x03"]
[0,7,"A","C","E",null,"VCR3    ",null,null,"subZone2","fncInput","eVCR3","\\x02","07ACE","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eVCR3","\\x0207ACE\\x03"]
[0,7,"A","D",8,null,"V-AUX    ",null,null,"subZone2","fncInput","eV_Aux","\\x02","07AD8","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncInput","AVRInterface::eV_Aux","\\x0207AD8\\x03"]
[0,7,"A",1,"D","Power","ON",null,20,"subMain","fncPower","eOn","\\x02","07A1D","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPower","AVRInterface::eOn","\\x0207A1D\\x03"]
[0,7,"A",1,"E",null,"OFF    ",null,null,"subMain","fncPower","eOff","\\x02","07A1E","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPower","AVRInterface::eOff","\\x0207A1E\\x03"]
[0,7,"E",7,"E","Main(Zone1) Power","ON",null,null,"subZone1","fncPower","eOn","\\x02","07E7E","\\x03",null,"AVRSubsys::subZone1","AVRFunc::fncPower","AVRInterface::eOn","\\x0207E7E\\x03"]
[0,7,"E",7,"F",null,"OFF    ",null,null,"subZone1","fncPower","eOff","\\x02","07E7F","\\x03",null,"AVRSubsys::subZone1","AVRFunc::fncPower","AVRInterface::eOff","\\x0207E7F\\x03"]
[0,7,"E","B","A","Zone2 power","ON",null,null,"subZone2","fncPower","eOn","\\x02","07EBA","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncPower","AVRInterface::eOn","\\x0207EBA\\x03"]
[0,7,"E","B","B",null,"OFF    ",null,null,"subZone2","fncPower","eOff","\\x02","07EBB","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncPower","AVRInterface::eOff","\\x0207EBB\\x03"]
[0,7,"A","E","D","Zone 3 Power ","ON",null,27,"subZone3","fncPower","eOn","\\x02","07AED","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncPower","AVRInterface::eOn","\\x0207AED\\x03"]
[0,7,"A","E","E",null,"STANDBY    ",null,null,"subZone3","fncPower","eStandby","\\x02","07AEE","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncPower","AVRInterface::eStandby","\\x0207AEE\\x03"]
[0,7,"E",2,6,"Zone 3 Mute ","ON",null,91,"subZone3","fncMute","eOn","\\x02","07E26","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncMute","AVRInterface::eOn","\\x0207E26\\x03"]
[0,7,"E",6,6,null,"OFF    ",null,null,"subZone3","fncMute","eOff","\\x02","07E66","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncMute","AVRInterface::eOff","\\x0207E66\\x03"]
[0,7,"A","F","D","Zone 3 Vol. ","UP",null,92,"subZone3","fncVolume","eUp","\\x02","07AFD","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncVolume","AVRInterface::eUp","\\x0207AFD\\x03"]
[0,7,"A","F","E",null,"DOWN    ",null,null,"subZone3","fncVolume","eDown","\\x02","07AFE","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncVolume","AVRInterface::eDown","\\x0207AFE\\x03"]
[0,7,"A","F",1,"Zone 3 Input ","PHONO",null,90,"subZone3","fncInput","ePhono","\\x02","07AF1","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::ePhono","\\x0207AF1\\x03"]
[0,7,"A","F",2,null,"CD    ",null,null,"subZone3","fncInput","eCD","\\x02","07AF2","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eCD","\\x0207AF2\\x03"]
[0,7,"A","F",3,null,"TUNER    ",null,null,"subZone3","fncInput","eTuner","\\x02","07AF3","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eTuner","\\x0207AF3\\x03"]
[0,7,"A","F",5,null,"CD-R    ",null,null,"subZone3","fncInput","eCDR","\\x02","07AF5","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eCDR","\\x0207AF5\\x03"]
[0,7,"A","F",4,null,"MD/TAPE    ",null,null,"subZone3","fncInput","eMD_Tape","\\x02","07AF4","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eMD_Tape","\\x0207AF4\\x03"]
[0,7,"A","F","C",null,"DVD    ",null,null,"subZone3","fncInput","eDVD","\\x02","07AFC","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eDVD","\\x0207AFC\\x03"]
[0,7,"A","F",6,null,"DTV/LD    ",null,null,"subZone3","fncInput","eDTV","\\x02","07AF6","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eDTV","\\x0207AF6\\x03"]
[0,7,"A","F",7,null,"CBL/SAT (cable)   ",null,null,"subZone3","fncInput","eCable","\\x02","07AF7","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eCable","\\x0207AF7\\x03"]
[0,7,"A","F",8,null,"SAT    ",null,null,"subZone3","fncInput","eSat","\\x02","07AF8","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eSat","\\x0207AF8\\x03"]
[0,7,"A","F",9,null,"VCR1    ",null,null,"subZone3","fncInput","eVCR1","\\x02","07AF9","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eVCR1","\\x0207AF9\\x03"]
[0,7,"A","F","A",null,"VCR2    ",null,null,"subZone3","fncInput","eVCR2_DVR","\\x02","07AFA","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eVCR2_DVR","\\x0207AFA\\x03"]
[0,7,"A","F","B",null,"DVR    ",null,null,"subZone3","fncInput","eVCR3","\\x02",{"$f":"A67&B67&C67&D67&E67","v":"07AFB"},"\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput",{"$f":"\"AVRInterface::\"&L67","v":"AVRInterface::eVCR3"},{"$f":"M67&N67&O67","v":"\\x0207AFB\\x03"}]
[0,7,"A","F",0,null,"V-AUX    ",null,null,"subZone3","fncInput","eV_Aux","\\x02","07AF0","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncInput","AVRInterface::eV_Aux","\\x0207AF0\\x03"]
[0,7,"E","B",0,"On screen(OSD)","OFF",null,"2B","subMain","fncOSD","eOSDOff","\\x02","07EB0","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncOSD","AVRInterface::eOSDOff","\\x0207EB0\\x03"]
[0,7,"E","B",1,null,"SHORT    ",null,null,"subMain","fncOSD","eOSDShort","\\x02","07EB1","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncOSD","AVRInterface::eOSDShort","\\x0207EB1\\x03"]
[0,7,"E","B",2,null,"FULL    ",null,null,"subMain","fncOSD","eOSDFull","\\x02","07EB2","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncOSD","AVRInterface::eOSDFull","\\x0207EB2\\x03"]
[0,7,"E","B",3,"Sleep","OFF  ",null,"2C","subMain","fncSleep","eSleepOff","\\x02","07EB3","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSleep","AVRInterface::eSleepOff","\\x0207EB3\\x03"]
[0,7,"E","B",4,null," 120   ",null,null,"subMain","fncSleep","eSleep120","\\x02","07EB4","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSleep","AVRInterface::eSleep120","\\x0207EB4\\x03"]
[0,7,"E","B",5,null," 90   ",null,null,"subMain","fncSleep","eSleep90","\\x02","07EB5","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSleep","AVRInterface::eSleep90","\\x0207EB5\\x03"]
[0,7,"E","B",6,null," 60   ",null,null,"subMain","fncSleep","eSleep60","\\x02","07EB6","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSleep","AVRInterface::eSleep60","\\x0207EB6\\x03"]
[0,7,"E","B",7,null," 30   ",null,null,"subMain","fncSleep","eSleep30","\\x02","07EB7","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSleep","AVRInterface::eSleep30","\\x0207EB7\\x03"]
[0,7,"E","B",8,"EX/ES ","ON (MATRIX) ",null,"2D","subMain","fncEx_EsOnOff","eOnMatrix","\\x02","07EB8","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEx_EsOnOff","AVRInterface::eOnMatrix","\\x0207EB8\\x03"]
[0,7,"E","B",9,null,"OFF    ",null,null,"subMain","fncEx_EsOnOff","eESESOff","\\x02","07EB9","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEx_EsOnOff","AVRInterface::eESESOff","\\x0207EB9\\x03"]
[0,7,"E",7,"C",null,"AUTO    ",null,null,"subMain","fncEx_EsOnOff","eAuto","\\x02","07E7C","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEx_EsOnOff","AVRInterface::eAuto","\\x0207E7C\\x03"]
[0,7,"E",7,"D",null,"DISCRETE    ",null,null,"subMain","fncEx_EsOnOff","eDiscrete","\\x02","07E7D","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEx_EsOnOff","AVRInterface::eDiscrete","\\x0207E7D\\x03"]
[0,7,"E",9,"B","Night mode","ON",null,82,"subMain","fncNightModeOnOff","eOn","\\x02","07E9B","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncNightModeOnOff","AVRInterface::eOn","\\x0207E9B\\x03"]
[0,7,"E",9,"C",null,"OFF   ",null,82,"subMain","fncNightModeOnOff","eOff","\\x02","07E9C","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncNightModeOnOff","AVRInterface::eOff","\\x0207E9C\\x03"]
[0,7,"E",2,7,"Effect ","ON",null,28,"subMain","fncEffect","eEffectOn","\\x02","07E27","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::eEffectOn","\\x0207E27\\x03"]
[0,7,"E","E",0,null,"Stereo    ",null,null,"subMain","fncEffect","eStereo","\\x02","07EE0","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::eStereo","\\x0207EE0\\x03"]
[0,7,"E","E",1,"DSP Program ","Hall A (Hall 1)",null,null,"subMain","fncEffect","Hall_A","\\x02","07EE1","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Hall_A","\\x0207EE1\\x03"]
[0,7,"E","E",2,null,"Hall B   ",null,null,"subMain","fncEffect","Hall_B","\\x02","07EE2","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Hall_B","\\x0207EE2\\x03"]
[0,7,"E","E",3,null,"Hall C   ",null,null,"subMain","fncEffect","Hall_C","\\x02","07EE3","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Hall_C","\\x0207EE3\\x03"]
[0,7,"E","E",4,null,"Hall U.S.A.   ",null,null,"subMain","fncEffect","Hall_USA","\\x02","07EE4","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Hall_USA","\\x0207EE4\\x03"]
[0,7,"E","E",5,null,"Hall E   ",null,null,"subMain","fncEffect","Hall_E","\\x02","07EE5","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Hall_E","\\x0207EE5\\x03"]
[0,7,"E","E",6,null,"Live Concert (HALL2 ) ",null,null,"subMain","fncEffect","Live_Concert","\\x02","07EE6","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Live_Concert","\\x0207EE6\\x03"]
[0,7,"E","E",7,null,"Tokyo    ",null,null,"subMain","fncEffect","Tokyo","\\x02","07EE7","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Tokyo","\\x0207EE7\\x03"]
[0,7,"E","E",8,null,"Freiburg ( CHURCH ) ",null,null,"subMain","fncEffect","Freiburg","\\x02","07EE8","\\x03",null,{"$f":"\"AVRSubsys::\" & J92","v":"AVRSubsys::subMain"},{"$f":"\"AVRFunc::\" & K92","v":"AVRFunc::fncEffect"},"AVRInterface::Freiburg","\\x0207EE8\\x03"]
[0,7,"E","E",9,null,"Royaumont    ",null,null,"subMain","fncEffect","Royaumont","\\x02","07EE9","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Royaumont","\\x0207EE9\\x03"]
[0,7,"E","E","A",null,"Village Gate   ",null,null,"subMain","fncEffect","Village_Gate","\\x02","07EEA","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Village_Gate","\\x0207EEA\\x03"]
[0,7,"E","E","B",null,"Village Vanguard   ",null,null,"subMain","fncEffect","Village_Vanguard","\\x02","07EEB","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Village_Vanguard","\\x0207EEB\\x03"]
[0,7,"E","E","C",null,"The Bottom Line ( JAZZ )",null,null,"subMain","fncEffect","The_Bottom_Line","\\x02","07EEC","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::The_Bottom_Line","\\x0207EEC\\x03"]
[0,7,"E","E","D",null,"The Roxy Theatre ( ROCK )",null,null,"subMain","fncEffect","The_Roxy_Theater","\\x02","07EED","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::The_Roxy_Theater","\\x0207EED\\x03"]
[0,7,"E","E","E",null,"Warehouse Loft   ",null,null,"subMain","fncEffect","Warehouse_Loft","\\x02","07EEE","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Warehouse_Loft","\\x0207EEE\\x03"]
[0,7,"E","E","F",null,"Arena    ",null,null,"subMain","fncEffect","Arena","\\x02","07EEF","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Arena","\\x0207EEF\\x03"]
[0,7,"E","F",0,null,"Disco    ",null,null,"subMain","fncEffect","Disco","\\x02","07EF0","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Disco","\\x0207EF0\\x03"]
[0,7,"E","F",1,null,"Party    ",null,null,"subMain","fncEffect","Party","\\x02","07EF1","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Party","\\x0207EF1\\x03"]
[0,7,"E","F",2,null,"Game    ",null,null,"subMain","fncEffect","Game","\\x02","07EF2","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Game","\\x0207EF2\\x03"]
[0,7,"E","F","F",null,"7ch Stereo   ",null,null,"subMain","fncEffect","Stereo_6_8Ch","\\x02","07EFF","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Stereo_6_8Ch","\\x0207EFF\\x03"]
[0,7,"E","F",3,null,"Pop/Rock ( Music Video) ",null,null,"subMain","fncEffect","Pop_Rock","\\x02","07EF3","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Pop_Rock","\\x0207EF3\\x03"]
[0,7,"E","F",4,null,"DJ    ",null,null,"subMain","fncEffect","DJ","\\x02","07EF4","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::DJ","\\x0207EF4\\x03"]
[0,7,"E","F",5,null,"Classical/Opera    ",null,null,"subMain","fncEffect","Opera","\\x02","07EF5","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Opera","\\x0207EF5\\x03"]
[0,7,"E","F",6,null,"Pavillion    ",null,null,"subMain","fncEffect","Pavillion","\\x02","07EF6","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Pavillion","\\x0207EF6\\x03"]
[0,7,"E","F",7,null,"Mono Movie   ",null,null,"subMain","fncEffect","Mono_Movie","\\x02","07EF7","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Mono_Movie","\\x0207EF7\\x03"]
[0,7,"E","F",8,null,"Variety Sports   ",null,null,"subMain","fncEffect","Variety_Sports","\\x02","07EF8","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Variety_Sports","\\x0207EF8\\x03"]
[0,7,"E","F",9,null,"Spectacle    ",null,null,"subMain","fncEffect","Spectacre","\\x02","07EF9","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Spectacre","\\x0207EF9\\x03"]
[0,7,"E","F","A",null,"Sci-Fi    ",null,null,"subMain","fncEffect","Sci_Fi","\\x02","07EFA","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Sci_Fi","\\x0207EFA\\x03"]
[0,7,"E","F","B",null,"Adventure    ",null,null,"subMain","fncEffect","Adventure","\\x02","07EFB","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Adventure","\\x0207EFB\\x03"]
[0,7,"E","F","C",null,"General    ",null,null,"subMain","fncEffect","General","\\x02","07EFC","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::General","\\x0207EFC\\x03"]
[0,7,"E","F","D",null,"Normal    ",null,null,"subMain","fncEffect","Normal","\\x02","07EFD","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Normal","\\x0207EFD\\x03"]
[0,7,"E","F","E",null,"Enhanced    ",null,null,"subMain","fncEffect","Enhanced","\\x02","07EFE","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Enhanced","\\x0207EFE\\x03"]
[0,7,"E",6,7,null,"PLII MOVIE   ",null,null,"subMain","fncEffect","PLII_Movie","\\x02","07E67","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::PLII_Movie","\\x0207E67\\x03"]
[0,7,"E",6,8,null,"PLII MUSIC   ",null,null,"subMain","fncEffect","PLII_Music","\\x02","07E68","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::PLII_Music","\\x0207E68\\x03"]
[0,7,"E",6,9,null,"NEO:6 CINEMA   ",null,null,"subMain","fncEffect","Neo_6_Movie","\\x02","07E69","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Neo_6_Movie","\\x0207E69\\x03"]
[0,7,"E",6,"A",null,"NEO:6 MUSIC   ",null,null,"subMain","fncEffect","Neo_6_Music","\\x02","07E6A","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","AVRInterface::Neo_6_Music","\\x0207E6A\\x03"]
[0,7,"E","C",1,null,"2CH DIRECT STEREO    ",null,null,"subMain","fncEffect","Direct_B_2Ch","\\x02","07EC1","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect",{"$f":"\"AVRInterface::\"&L124","v":"AVRInterface::THX_Ultra_PL"},"\\x0207EC1\\x03"]
[0,7,"E","C",0,null,"2CH STEREO   ",null,null,"subMain","fncEffect","Stereo_A_2Ch","\\x02","07EC0","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect",{"$f":"\"AVRInterface::\"&L125","v":"AVRInterface::THX_Ultra_NEO6"},"\\x0207EC0\\x03"]
[0,7,"E","C",2,null,"THX (ULTRA2) CINEMA + PL    ",null,null,"subMain","fncEffect","THX_Ultra_PL","\\x02","07EC2","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect",{"$f":"\"AVRInterface::\"&L121","v":"AVRInterface::Stereo_A_2Ch"},"\\x0207EC2\\x03"]
[0,7,"E","C",3,null,"THX MUSIC MUSIC   ",null,null,"subMain","fncEffect","THX_Musit","\\x02","07EC3","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect",{"$f":"\"AVRInterface::\"&L120","v":"AVRInterface::Direct_B_2Ch"},"\\x0207EC3\\x03"]
[0,7,"E","C",7,null,"THX (ULTRA2) CINEMA + PL2    ",null,null,"subMain","fncEffect","THX_Ultra_PL","\\x02","07EC7","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect","vvvvv","\\x0207EC7\\x03"]
[0,7,"E","C",8,null,"THX (ULTRA2) CINEMA + NEO6    ",null,null,"subMain","fncEffect","THX_Ultra_NEO6","\\x02","07EC8","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncEffect",{"$f":"\"AVRInterface::\"&L122","v":"AVRInterface::THX_Ultra_PL"},"\\x0207EC8\\x03"]
[0,7,"A","E",0,"Tuner preset page","A",0,29,"subMain","fncPresetPage","eA","\\x02","07AE0","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetPage","AVRInterface::eA","\\x0207AE0\\x03"]
[0,7,"A","E",1,null,"B    ",null,null,"subMain","fncPresetPage","eB","\\x02","07AE1","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetPage","AVRInterface::eB","\\x0207AE1\\x03"]
[0,7,"A","E",2,null,"C    ",null,null,"subMain","fncPresetPage","eC","\\x02","07AE2","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetPage","AVRInterface::eC","\\x0207AE2\\x03"]
[0,7,"A","E",3,null,"D    ",null,null,"subMain","fncPresetPage","eD","\\x02","07AE3","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetPage","AVRInterface::eD","\\x0207AE3\\x03"]
[0,7,"A","E",4,null,"E    ",null,null,"subMain","fncPresetPage","eE","\\x02","07AE4","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetPage","AVRInterface::eE","\\x0207AE4\\x03"]
[0,7,"A","E",5,"Tuner preset No.",1,null,"2A","subMain","fncPresetNum","e1","\\x02",{"$f":"A131&B131&C131&D131&E131","v":"07AE5"},"\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum",{"$f":"\"AVRInterface::\"&L131","v":"AVRInterface::e1"},{"$f":"M131&N131&O131","v":"\\x0207AE5\\x03"}]
[0,7,"A","E",6,null,"2    ",null,null,"subMain","fncPresetNum","e2","\\x02","07AE6","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e2","\\x0207AE6\\x03"]
[0,7,"A","E",7,null,"3    ",null,null,"subMain","fncPresetNum","e3","\\x02","07AE7","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e3","\\x0207AE7\\x03"]
[0,7,"A","E",8,null,"4    ",null,null,"subMain","fncPresetNum","e4","\\x02","07AE8","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e4","\\x0207AE8\\x03"]
[0,7,"A","E",9,null,"5    ",null,null,"subMain","fncPresetNum","e5","\\x02","07AE9","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e5","\\x0207AE9\\x03"]
[0,7,"A","E","A",null,"6    ",null,null,"subMain","fncPresetNum","e6","\\x02","07AEA","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e6","\\x0207AEA\\x03"]
[0,7,"A","E","B",null,"7    ",null,null,"subMain","fncPresetNum","e7","\\x02","07AEB","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e7","\\x0207AEB\\x03"]
[0,7,"A","E","C",null,"8    ",null,null,"subMain","fncPresetNum","e8","\\x02","07AEC","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncPresetNum","AVRInterface::e8","\\x0207AEC\\x03"]
[0,7,"E","B","C","Tuner band ","FM ",null,35,"subMain","fncRadioBand","eFM","\\x02","07EBC","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioBand","AVRInterface::eFM","\\x0207EBC\\x03"]
[0,7,"E","B","D",null,"AM    ",null,null,"subMain","fncRadioBand","eAM","\\x02","07EBD","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioBand","AVRInterface::eAM","\\x0207EBD\\x03"]
[0,7,"E","B","E","Auto tuning start ","UP",null,15,"subMain","fncRadioTune","eUp","\\x02","07EBE","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioTune","AVRInterface::eUp","\\x0207EBE\\x03"]
[0,7,"E","B","F",null,"DOWN    ",null,null,"subMain","fncRadioTune","eDown","\\x02","07EBF","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioTune","AVRInterface::eDown","\\x0207EBF\\x03"]
[0,7,"E","A","B","speaker relay A","ON",null,"2E","subMain","fncSpeakerAOnOff","eOn","\\x02","07EAB","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSpeakerAOnOff","AVRInterface::eOn","\\x0207EAB\\x03"]
[0,7,"E","A","C",null,"OFF    ",null,null,"subMain","fncSpeakerAOnOff","eOff","\\x02","07EAC","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSpeakerAOnOff","AVRInterface::eOff","\\x0207EAC\\x03"]
[0,7,"E","A","D","speaker relay B","ON",null,"2F","subMain","fncSpeakerBOnOff","eOn","\\x02","07EAD","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSpeakerBOnOff","AVRInterface::eOn","\\x0207EAD\\x03"]
[0,7,"E","A","E",null,"OFF    ",null,null,"subMain","fncSpeakerBOnOff","eOff","\\x02","07EAE","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncSpeakerBOnOff","AVRInterface::eOff","\\x0207EAE\\x03"]
[0,7,"E",2,"B","Home preset memory","A",null,null,"subMain","fncRadioPresetMemory","eA","\\x02","07E2B","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetMemory","AVRInterface::eA","\\x0207E2B\\x03"]
[0,7,"E",2,"C",null,"B    ",null,null,"subMain","fncRadioPresetMemory","eB","\\x02","07E2C","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetMemory","AVRInterface::eB","\\x0207E2C\\x03"]
[0,7,"E",2,"D",null,"C    ",null,null,"subMain","fncRadioPresetMemory","eC","\\x02","07E2D","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetMemory","AVRInterface::eC","\\x0207E2D\\x03"]
[0,7,"E",2,"E",null,"D    ",null,null,"subMain","fncRadioPresetMemory","eD","\\x02","07E2E","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetMemory","AVRInterface::eD","\\x0207E2E\\x03"]
[0,7,"E",2,"F",null,"E    ",null,null,"subMain","fncRadioPresetMemory","eE","\\x02","07E2F","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetMemory","AVRInterface::eE","\\x0207E2F\\x03"]
[0,7,"E",2,0,null,"F    ",null,null,"subMain","fncRadioPresetMemory","eF","\\x02","07E20","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetMemory","AVRInterface::eF","\\x0207E20\\x03"]
[0,7,"E",3,5,"Home preset recall","A ",null,null,"subMain","fncRadioPresetRecall","eA","\\x02","07E35","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetRecall","AVRInterface::eA","\\x0207E35\\x03"]
[0,7,"E",3,6,null,"B",null,null,"subMain","fncRadioPresetRecall","eB","\\x02","07E36","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetRecall","AVRInterface::eB","\\x0207E36\\x03"]
[0,7,"E",3,7,null,"C",null,31,"subMain","fncRadioPresetRecall","eC","\\x02","07E37","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetRecall","AVRInterface::eC","\\x0207E37\\x03"]
[0,7,"E",3,8,null,"D",null,null,"subMain","fncRadioPresetRecall","eD","\\x02","07E38","\\x03",null,{"$f":"\"AVRSubsys::\" & J156","v":"AVRSubsys::subMain"},{"$f":"\"AVRFunc::\" & K156","v":"AVRFunc::fncRadioPresetRecall"},"AVRInterface::eD","\\x0207E38\\x03"]
[0,7,"E",3,9,null,"E",null,null,"subMain","fncRadioPresetRecall","eE","\\x02","07E39","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetRecall","AVRInterface::eE","\\x0207E39\\x03"]
[0,7,"E",3,"A",null,"F",null,null,"subMain","fncRadioPresetRecall","eF","\\x02","07E3A","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncRadioPresetRecall","AVRInterface::eF","\\x0207E3A\\x03"]
[0,7,"E",6,"B","Volume preset memory ","A ",null,null,"subMain","fncVolumeMemory","eA","\\x02","07E6B","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeMemory","AVRInterface::eA","\\x0207E6B\\x03"]
[0,7,"E",6,"C",null,"B    ",null,null,"subMain","fncVolumeMemory","eB","\\x02","07E6C","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeMemory","AVRInterface::eB","\\x0207E6C\\x03"]
[0,7,"E",6,"D",null,"C    ",null,null,"subMain","fncVolumeMemory","eC","\\x02","07E6D","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeMemory","AVRInterface::eC","\\x0207E6D\\x03"]
[0,7,"E",6,"E",null,"D    ",null,null,"subMain","fncVolumeMemory","eD","\\x02","07E6E","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeMemory","AVRInterface::eD","\\x0207E6E\\x03"]
[0,7,"E",6,"F",null,"E    ",null,null,"subMain","fncVolumeMemory","eE","\\x02","07E6F","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeMemory","AVRInterface::eE","\\x0207E6F\\x03"]
[0,7,"E",6,0,null,"F    ",null,null,"subMain","fncVolumeMemory","eF","\\x02","07E60","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeMemory","AVRInterface::eF","\\x0207E60\\x03"]
[0,7,"E",7,5,"Volume preset recall","A",null,null,"subMain","fncVolumeRecall","eA","\\x02","07E75","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeRecall","AVRInterface::eA","\\x0207E75\\x03"]
[0,7,"E",7,6,null,"B    ",null,null,"subMain","fncVolumeRecall","eB","\\x02","07E76","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeRecall","AVRInterface::eB","\\x0207E76\\x03"]
[0,7,"E",7,7,null,"C    ",null,null,"subMain","fncVolumeRecall","eC","\\x02","07E77","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeRecall","AVRInterface::eC","\\x0207E77\\x03"]
[0,7,"E",7,8,null,"D    ",null,null,"subMain","fncVolumeRecall","eD","\\x02","07E78","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeRecall","AVRInterface::eD","\\x0207E78\\x03"]
[0,7,"E",7,9,null,"E    ",null,null,"subMain","fncVolumeRecall","eE","\\x02","07E79","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeRecall","AVRInterface::eE","\\x0207E79\\x03"]
[0,7,"E",7,"A",null,"F    ",null,null,"subMain","fncVolumeRecall","eF","\\x02","07E7A","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncVolumeRecall","AVRInterface::eF","\\x0207E7A\\x03"]
[0,7,"E",8,7,"Z2 Vol. Memory ","A ",null,null,"subZone2","fncVolumeMemory","eA","\\x02","07E87","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeMemory","AVRInterface::eA","\\x0207E87\\x03"]
[0,7,"E",8,8,null,"B    ",null,null,"subZone2","fncVolumeMemory","eB","\\x02","07E88","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeMemory","AVRInterface::eB","\\x0207E88\\x03"]
[0,7,"E",8,9,null,"C    ",null,null,"subZone2","fncVolumeMemory","eC","\\x02","07E89","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeMemory","AVRInterface::eC","\\x0207E89\\x03"]
[0,7,"E",8,"A",null,"D    ",null,null,"subZone2","fncVolumeMemory","eD","\\x02","07E8A","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeMemory","AVRInterface::eD","\\x0207E8A\\x03"]
[0,7,"E",8,"B",null,"E    ",null,null,"subZone2","fncVolumeMemory","eE","\\x02","07E8B","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeMemory","AVRInterface::eE","\\x0207E8B\\x03"]
[0,7,"E",8,"C",null,"F    ",null,null,"subZone2","fncVolumeMemory","eF","\\x02","07E8C","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeMemory","AVRInterface::eF","\\x0207E8C\\x03"]
[0,7,"E",8,"D","Z2 Vol. Recall ","A ",null,null,"subZone2","fncVolumeRecall","eA","\\x02","07E8D","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeRecall","AVRInterface::eA","\\x0207E8D\\x03"]
[0,7,"E",8,"E",null,"B    ",null,null,"subZone2","fncVolumeRecall","eB","\\x02","07E8E","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeRecall","AVRInterface::eB","\\x0207E8E\\x03"]
[0,7,"E",8,"F",null,"C    ",null,null,"subZone2","fncVolumeRecall","eC","\\x02","07E8F","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeRecall","AVRInterface::eC","\\x0207E8F\\x03"]
[0,7,"E",9,0,null,"D    ",null,null,"subZone2","fncVolumeRecall","eD","\\x02","07E90","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeRecall","AVRInterface::eD","\\x0207E90\\x03"]
[0,7,"E",9,1,null,"E    ",null,null,"subZone2","fncVolumeRecall","eE","\\x02","07E91","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeRecall","AVRInterface::eE","\\x0207E91\\x03"]
[0,7,"E",9,2,null,"F    ",null,null,"subZone2","fncVolumeRecall","eF","\\x02","07E92","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncVolumeRecall","AVRInterface::eF","\\x0207E92\\x03"]
[0,7,"E",2,0,"Z3 Vol. Memory ","A ",null,94,"subZone3","fncVolumeMemory","eA","\\x02","07E20","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncVolumeMemory","AVRInterface::eA","\\x0207E20\\x03"]
[0,7,"E",2,1,null,"B    ",null,null,"subZone4","fncVolumeMemory","eB","\\x02","07E21","\\x03",null,"AVRSubsys::subZone4","AVRFunc::fncVolumeMemory","AVRInterface::eB","\\x0207E21\\x03"]
[0,7,"E",2,2,null,"C    ",null,null,"subZone5","fncVolumeMemory","eC","\\x02","07E22","\\x03",null,"AVRSubsys::subZone5","AVRFunc::fncVolumeMemory","AVRInterface::eC","\\x0207E22\\x03"]
[0,7,"E",2,3,null,"D    ",null,null,"subZone6","fncVolumeMemory","eD","\\x02","07E23","\\x03",null,"AVRSubsys::subZone6","AVRFunc::fncVolumeMemory","AVRInterface::eD","\\x0207E23\\x03"]
[0,7,"E",2,4,null,"E    ",null,null,"subZone7","fncVolumeMemory","eE","\\x02","07E24","\\x03",null,"AVRSubsys::subZone7","AVRFunc::fncVolumeMemory","AVRInterface::eE","\\x0207E24\\x03"]
[0,7,"E",2,5,null,"F    ",null,null,"subZone8","fncVolumeMemory","eF","\\x02","07E25","\\x03",null,"AVRSubsys::subZone8","AVRFunc::fncVolumeMemory","AVRInterface::eF","\\x0207E25\\x03"]
[0,7,"E",6,0,"Z3 Vol. Recall ","A ",null,93,"subZone9","fncVolumeRecall","eA","\\x02","07E60","\\x03",null,"AVRSubsys::subZone9","AVRFunc::fncVolumeRecall","AVRInterface::eA","\\x0207E60\\x03"]
[0,7,"E",6,1,null,"B    ",null,null,"subZone10","fncVolumeRecall","eB","\\x02","07E61","\\x03",null,"AVRSubsys::subZone10","AVRFunc::fncVolumeRecall","AVRInterface::eB","\\x0207E61\\x03"]
[0,7,"E",6,2,null,"C    ",null,null,"subZone11","fncVolumeRecall","eC","\\x02","07E62","\\x03",null,"AVRSubsys::subZone11","AVRFunc::fncVolumeRecall","AVRInterface::eC","\\x0207E62\\x03"]
[0,7,"E",6,3,null,"D    ",null,null,"subZone12","fncVolumeRecall","eD","\\x02","07E63","\\x03",null,"AVRSubsys::subZone12","AVRFunc::fncVolumeRecall","AVRInterface::eD","\\x0207E63\\x03"]
[0,7,"E",6,4,null,"E    ",null,null,"subZone13","fncVolumeRecall","eE","\\x02","07E64","\\x03",null,"AVRSubsys::subZone13","AVRFunc::fncVolumeRecall","AVRInterface::eE","\\x0207E64\\x03"]
[0,7,"E",6,5,null,"F    ",null,null,"subZone14","fncVolumeRecall","eF","\\x02","07E65","\\x03",null,"AVRSubsys::subZone14","AVRFunc::fncVolumeRecall","AVRInterface::eF","\\x0207E65\\x03"]
[0,7,"E",3,2,"DC1 TRG Control  ","Zone 1",null,"3A","subMain","fncDC1TrigControl","eZone1","\\x02",{"$f":"A195&B195&C195&D195&E195","v":"07E32"},"\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl",{"$f":"\"AVRInterface::\"&L195","v":"AVRInterface::eZone1"},{"$f":"M195&N195&O195","v":"\\x0207E32\\x03"}]
[0,7,"E",3,3,null,"Zone 2   ",null,null,"subMain","fncDC1TrigControl","eZone2","\\x02","07E33","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl","AVRInterface::eZone2","\\x0207E33\\x03"]
[0,7,"E",3,1,null,"Zone 3   ",null,null,"subMain","fncDC1TrigControl","eZone3","\\x02","07E31","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl","AVRInterface::eZone3","\\x0207E31\\x03"]
[0,7,"E",7,1,"Zone 2 DC1 TRG","On",null,36,"subZone2","fncDC1OnOff","eOn","\\x02","07E71","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncDC1OnOff","AVRInterface::eOn","\\x0207E71\\x03"]
[0,7,"E",7,2,null,"Off    ",null,null,"subZone2","fncDC1OnOff","eOff","\\x02","07E72","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncDC1OnOff","AVRInterface::eOff","\\x0207E72\\x03"]
[0,7,"E",7,3,"Zone 1 DC1 TRG","On",null,36,"subZone1","fncDC1OnOff","eOn","\\x02","07E73","\\x03",null,"AVRSubsys::subZone1","AVRFunc::fncDC1OnOff","AVRInterface::eOn","\\x0207E73\\x03"]
[0,7,"E",7,4,null,"Off    ",null,null,"subZone1","fncDC1OnOff","eOff","\\x02","07E74","\\x03",null,"AVRSubsys::subZone1","AVRFunc::fncDC1OnOff","AVRInterface::eOff","\\x0207E74\\x03"]
[0,7,"E",8,3,"Zone 3 DC1 TRG","On",null,36,"subZone3","fncDC1OnOff","eOn","\\x02","07E83","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncDC1OnOff","AVRInterface::eOn","\\x0207E83\\x03"]
[0,7,"E",8,4,null,"Off    ",null,null,"subZone3","fncDC1OnOff","eOff","\\x02","07E84","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncDC1OnOff","AVRInterface::eOff","\\x0207E84\\x03"]
[0,7,"E",9,3,"Dual Mono   ","Main",null,39,"subMain","fncDualMono","eMain","\\x02","07E93","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDualMono","AVRInterface::eMain","\\x0207E93\\x03"]
[0,7,"E",9,4,null,"Sub    ",null,null,"subMain","fncDualMono","eSub","\\x02","07E94","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDualMono","AVRInterface::eSub","\\x0207E94\\x03"]
[0,7,"E",9,5,null,"All    ",null,null,"subMain","fncDualMono","eAll","\\x02","07E95","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDualMono","AVRInterface::eAll","\\x0207E95\\x03"]
[0,7,"E",9,6,"DC2 TRG Control","Zone 1",null,"3B","subMain","fncDC1TrigControl","eZone1","\\x02","07E96","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl","AVRInterface::eZone1","\\x0207E96\\x03"]
[0,7,"E",9,7,null,"Zone 2   ",null,null,"subMain","fncDC1TrigControl","eZone2","\\x02","07E97","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl","AVRInterface::eZone2","\\x0207E97\\x03"]
[0,7,"E",9,"F",null,"Zone 3   ",null,null,"subMain","fncDC1TrigControl","eZone3","\\x02","07E9F","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl","AVRInterface::eZone3","\\x0207E9F\\x03"]
[0,7,"E",9,8,null,"Zone OR   ",null,null,"subMain","fncDC1TrigControl","eZoneOR","\\x02","07E98","\\x03",null,"AVRSubsys::subMain","AVRFunc::fncDC1TrigControl","AVRInterface::eZoneOR","\\x0207E98\\x03"]
[0,7,"E",3,"C","Zone 2 DC2 TRG","On",null,"3C","subZone2","fncDC2OnOff","eOn","\\x02","07E3C","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncDC2OnOff","AVRInterface::eOn","\\x0207E3C\\x03"]
[0,7,"E",3,"D",null,"Off    ",null,null,"subZone2","fncDC2OnOff","eOff","\\x02","07E3D","\\x03",null,"AVRSubsys::subZone2","AVRFunc::fncDC2OnOff","AVRInterface::eOff","\\x0207E3D\\x03"]
[0,7,"E",3,"E","Zone 1 DC2 TRG","On",null,"3C","subZone1","fncDC2OnOff","eOn","\\x02","07E3E","\\x03",null,"AVRSubsys::subZone1","AVRFunc::fncDC2OnOff","AVRInterface::eOn","\\x0207E3E\\x03"]
[0,7,"E",3,"F",null,"Off    ",null,null,"subZone1","fncDC2OnOff","eOff","\\x02","07E3F","\\x03",null,"AVRSubsys::subZone1","AVRFunc::fncDC2OnOff","AVRInterface::eOff","\\x0207E3F\\x03"]
[0,7,"E",8,5,"Zone 3 DC2 TRG","On",null,"3C","subZone3","fncDC2OnOff","eOn","\\x02","07E85","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncDC2OnOff","AVRInterface::eOn","\\x0207E85\\x03"]
[0,7,"E",8,6,null,"Off    ",null,null,"subZone3","fncDC2OnOff","eOff","\\x02","07E86","\\x03",null,"AVRSubsys::subZone3","AVRFunc::fncDC2OnOff","AVRInterface::eOff","\\x0207E86\\x03"]
[0,7,"E",2,8,"SP B SET","Zone 1",null,"3E","subMain","speakerBZone","eZone1","\\x02","07E28","\\x03",null,"AVRSubsys::subMain","AVRFunc::speakerBZone","AVRInterface::eZone1","\\x0207E28\\x03"]
[0,7,"E",2,9,null,"Zone 2   ",null,null,"subMain","speakerBZone","eZone2","\\x02","07E29","\\x03",null,"AVRSubsys::subMain","AVRFunc::speakerBZone","AVRInterface::eZone2","\\x0207E29\\x03"]
[0,7,"E",9,9,"Zone SP OUT","On",null,"3F (70/73/78)","subMain","zone2Speaker","eOn","\\x02","07E99","\\x03",null,"AVRSubsys::subMain","AVRFunc::zone2Speaker","AVRInterface::eOn","\\x0207E99\\x03"]
[0,7,"E",9,"A",null,"Off",null,null,"subMain","zone2Speaker","eOff","\\x02","07E9A","\\x03",null,{"$f":"\"AVRSubsys::\" & J220","v":"AVRSubsys::subMain"},{"$f":"\"AVRFunc::\" & K220","v":"AVRFunc::zone2Speaker"},"AVRInterface::eOff","\\x0207E9A\\x03"]

{"sheet":"Sheet1","index":2,"n_rows":44,"n_cols":92,"rows_kept":44}
["master volume","Up","Zone 2 Volume ","UP","Zone 3 Vol. ","UP","Auto tuning start ","UP","Audio Mute","ON","6ch input","ON","Zone2 mute","ON","Power","ON","Main(Zone1) Power","ON","Zone2 power","ON","Zone 3 Mute ","ON","Night mode","ON","Zone 2 DC1 TRG","On","Zone 1 DC1 TRG","On","Zone 3 DC1 TRG","On","Zone 2 DC2 TRG","On","Zone 1 DC2 TRG","On","Zone 3 DC2 TRG","On","Zone SP OUT","On","speaker relay A","ON","speaker relay B","ON","Zone 3 Power ","ON","On screen(OSD)","OFF","Sleep","OFF  ","EX/ES ","ON (MATRIX) ","Effect ","ON","Tuner preset No.",1,"Tuner band ","FM ","Tuner preset page","A","Home preset memory","A","Home preset recall","A ","Volume preset memory ","A ","Volume preset recall","A","Z2 Vol. Memory ","A ","Z2 Vol. Recall ","A ","Z3 Vol. Memory ","A ","Z3 Vol. Recall ","A ","Input  ","PHONO","Zone2 Input","PHONO","Zone 3 Input ","PHONO","Input Mode ","AUTO","Dual Mono   ","Main","DC1 TRG Control  ","Zone 1","DC2 TRG Control","Zone 1","SP B SET","Zone 1","DSP Program ","Hall A (Hall 1)"]
[null,"Down    ",null,"DOWN    ",null,"DOWN    ",null,"DOWN    ",null,"OFF    ",null,"OFF    ",null,"OFF    ",null,"OFF    ",null,"OFF    ",null,"OFF    ",null,"OFF    ",null,"OFF   ",null,"Off    ",null,"Off    ",null,"Off    ",null,"Off    ",null,"Off    ",null,"Off    ",null,"Off",null,"OFF    ",null,"OFF    ",null,"STANDBY    ",null,"SHORT    ",null," 120   ",null,"OFF    ",null,"Stereo    ",null,"2    ",null,"AM    ",null,"B    ",null,"B    ",null,"B",null,"B    ",null,"B    ",null,"B    ",null,"B    ",null,"B    ",null,"B    ",null,"CD    ",null,"CD    ",null,"CD    ",null,"D.D., RF   ",null,"Sub    ",null,"Zone 2   ",null,"Zone 2   ",null,"Zone 2   ",null,"Hall B   "]
[{"$nulls":45},"FULL    ",null," 90   ",null,"AUTO    ",{"$nulls":3},"3    ",{"$nulls":3},"C    ",null,"C    ",null,"C",null,"C    ",null,"C    ",null,"C    ",null,"C    ",null,"C    ",null,"C    ",null,"TUNER    ",null,"TUNER    ",null,"TUNER    ",null,"DTS    ",null,"All    ",null,"Zone 3   ",null,"Zone 3   ",{"$nulls":3},"Hall C   "]
[{"$nulls":47}," 60   ",null,"DISCRETE    ",{"$nulls":3},"4    ",{"$nulls":3},"D    ",null,"D    ",null,"D",null,"D    ",null,"D    ",null,"D    ",null,"D    ",null,"D    ",null,"D    ",null,"CD-R    ",null,"CD-R    ",null,"CD-R    ",null,"DIGITAL    ",{"$nulls":5},"Zone OR   ",{"$nulls":3},"Hall U.S.A.   "]
[{"$nulls":47}," 30   ",{"$nulls":5},"5    ",{"$nulls":3},"E    ",null,"E    ",null,"E",null,"E    ",null,"E    ",null,"E    ",null,"E    ",null,"E    ",null,"E    ",null,"MD/TAPE    ",null,"MD/TAPE    ",null,"MD/TAPE    ",null,"ANALOG    ",{"$nulls":9},"Hall E   "]
[{"$nulls":53},"6    ",{"$nulls":5},"F    ",null,"F",null,"F    ",null,"F    ",null,"F    ",null,"F    ",null,"F    ",null,"F    ",null,"DVD    ",null,"DVD    ",null,"DVD    ",null,"AAC    ",{"$nulls":9},"Live Concert (HALL2 ) "]
[{"$nulls":53},"7    ",{"$nulls":21},"D-TV/LD    ",null,"D-TV/LD    ",null,"DTV/LD    ",{"$nulls":11},"Tokyo    "]
["Zone 1/Master","On","Off","Up","Down","Mute","UnMute","DC1 Trigger On","DC1 Trigger Off","DC2 Trig On","DC2 Trigger Off","Speaker A On","Speaker A Off","Speaker B On","Speaker B Off","PHONO","CD    ","TUNER    ","CD-R    ","MD/TAPE    ","DVD    ","D-TV/LD    ","CABLE ( CBL/SAT ) ","SAT    ","VCR1    ","VCR2/DVR    ","VCR3    ","V-AUX    ",{"$nulls":25},"8    ",{"$nulls":21},"CABLE ( CBL/SAT ) ",null,"CABLE ( CBL/SAT ) ",null,"CBL/SAT (cable)   ",{"$nulls":11},"Freiburg ( CHURCH ) "]
["Zone 2","On","Off","Up","Down","Mute","UnMute","DC1 Trigger On","DC1 Trigger Off","DC2 Trig On","DC2 Trigger Off","Speaker On","Speaker Off",null,null,"PHONO","CD    ","TUNER    ","CD-R    ","MD/TAPE    ","DVD    ","D-TV/LD    ","CABLE ( CBL/SAT ) ","SUN","VCR2","VCR2/DVR    ","VCR4","V-AUX    ",{"$nulls":47},"SAT    ",null,"SAT    ",null,"SAT    ",{"$nulls":11},"Royaumont    "]
["Zone 3","On","Off","Up","Down","Mute","UnMute","DC1 Trigger On","DC1 Trigger Off","DC2 Trig On","DC2 Trigger Off",{"$nulls":4},"PHONO","CD    ","TUNER    ","CD-R    ","MD/TAPE    ","DVD    ","D-TV/LD    ","CABLE ( CBL/SAT ) ","MON","VCR3","VCR2/DVR    ","VCR5","V-AUX    ",{"$nulls":47},"VCR1    ",null,"VCR1    ",null,"VCR1    ",{"$nulls":11},"Village Gate   "]
["Speaker B Set","Zone 1","Zone 2"]
["Night Mode","On","Off"]
["DC1 Trig Control","Zone 1","Zone 2","Zone 3"]
["DC2 TrigControl","Zone 1","Zone 2","Zone 3","Zone OR",{"$nulls":70},"VCR2/DVR    ",null,"VCR2/DVR    ",null,"VCR2    ",{"$nulls":11},"Village Vanguard   "]
[{"$nulls":75},"VCR3    ",null,"VCR3    ",null,"DVR    ",{"$nulls":11},"The Bottom Line ( JAZZ )"]
["6 Ch Input","On","Off",{"$nulls":72},"V-AUX    ",null,"V-AUX    ",null,"V-AUX    ",{"$nulls":11},"The Roxy Theatre ( ROCK )"]
["EX_ES","On(Matrix)","Off","Auto","Discrete",{"$nulls":86},"Warehouse Loft   "]
["Effect","On","Stereo",{"$nulls":88},"Arena    "]
["Input Mode","AUTO","D.D., RF   ","DTS    ","DIGITAL    ","ANALOG    ","AAC    ",{"$nulls":84},"Disco    "]
["Dual Mono","Main","Sub","All",{"$nulls":87},"Party    "]
[{"$nulls":91},"Game    "]
[{"$nulls":91},"7ch Stereo   "]
["DSP Program","Hall A (Hall 1)","Hall B   ","Hall C   ","Hall U.S.A.   ","Hall E   ","Live Concert (HALL2 ) ","Tokyo    ","Freiburg ( CHURCH ) ","Royaumont    ","Village Gate   ","Village Vanguard   ","The Bottom Line ( JAZZ )","The Roxy Theatre ( ROCK )","Warehouse Loft   ","Arena    ","Disco    ","Party    ","Game    ","7ch Stereo   ","Pop/Rock ( Music Video) ","DJ    ","Classical/Opera    ","Pavillion    ","Mono Movie   ","Variety Sports   ","Spectacle    ","Sci-Fi    ","Adventure    ","General    ","Normal    ","Enhanced    ","PLII MOVIE   ","PLII MUSIC   ","NEO:6 CINEMA   ","NEO:6 MUSIC   ","2CH DIRECT STEREO    ","2CH STEREO   ","THX (ULTRA2) CINEMA + PL    ","THX MUSIC MUSIC   ","THX (ULTRA2) CINEMA + PL2    ","THX (ULTRA2) CINEMA + NEO6    ",{"$nulls":49},"Pop/Rock ( Music Video) "]
[{"$nulls":91},"DJ    "]
["OSD","Off","Short","Full",{"$nulls":87},"Classical/Opera    "]
["Sleep","Off",120,90,60,30,{"$nulls":85},"Pavillion    "]
[{"$nulls":91},"Mono Movie   "]
[{"$nulls":91},"Variety Sports   "]
["Band","FM","AM",{"$nulls":88},"Spectacle    "]
["Auto Tuning","Up","Down",{"$nulls":88},"Sci-Fi    "]
["Tuner Preset Page","A","B","C","D","E",{"$nulls":85},"Adventure    "]
["Home preset memory","A","B","C","D","E","F",{"$nulls":84},"General    "]
["Home preset recall","A","B","C","D","E","F",{"$nulls":84},"Normal    "]
["Volume preset memory ","A","B","C","D","E","F",{"$nulls":84},"Enhanced    "]
["Volume preset recall","A","B","C","D","E","F",{"$nulls":84},"PLII MOVIE   "]
["Z2 Vol. Memory ","A","B","C","D","E","F",{"$nulls":84},"PLII MUSIC   "]
["Z2 Vol. Recall ","A","B","C","D","E","F",{"$nulls":84},"NEO:6 CINEMA   "]
["Z3 Vol. Memory ","A","B","C","D","E","F",{"$nulls":84},"NEO:6 MUSIC   "]
["Z3 Vol. Recall ","A","B","C","D","E","F",{"$nulls":84},"2CH DIRECT STEREO    "]
["Tuner Preset Number",1,2,3,4,5,6,7,8,{"$nulls":82},"2CH STEREO   "]
[{"$nulls":91},"THX (ULTRA2) CINEMA + PL    "]
[{"$nulls":91},"THX MUSIC MUSIC   "]
[{"$nulls":91},"THX (ULTRA2) CINEMA + PL2    "]
[{"$nulls":91},"THX (ULTRA2) CINEMA + NEO6    "]

{"sheet":"System Status","index":3,"n_rows":459,"n_cols":5,"rows_kept":459}
["Report Type","RCMD0, 0","Report Item","RDAT0,1","Status"]
["System","00","system","00","OK"]
[{"$nulls":3},"01","Busy"]
[{"$nulls":3},"02","Power Off"]
[{"$nulls":3},"03"]
[{"$nulls":3},"04"]
[{"$nulls":3},"05"]
[{"$nulls":3},"06"]
[{"$nulls":3},"07"]
["Status","10","Playback","00","6CH Input"]
[{"$nulls":3},"01","Analog"]
[{"$nulls":3},"02","PCM"]
[{"$nulls":3},"03","D.D.(except for 2/0)"]
[{"$nulls":3},"04","D.D.(2/0)"]
[{"$nulls":3},"05","D.D.karaoke"]
[{"$nulls":3},"06","D.D.EX"]
[{"$nulls":3},"07","DTS"]
[{"$nulls":3},"08","DTS. ES"]
[{"$nulls":3},"09","Other Digital"]
[{"$nulls":3},"0A","DTS Analog Mute"]
[{"$nulls":3},"0B","DTS Discrete"]
[{"$nulls":3},"0C","Other than AAC 2/0"]
[{"$nulls":3},"0D","AAC 2/0"]
[null,"11","Fs","00","Analog"]
[{"$nulls":3},"01","32kHz"]
[{"$nulls":3},"02","44.1kHz"]
[{"$nulls":3},"03","48kHz"]
[{"$nulls":3},"04","64kHz"]
[{"$nulls":3},"05","88.2kHz"]
[{"$nulls":3},"06","96kHz"]
[{"$nulls":3},"07","Unknown"]
[{"$nulls":3},"08","128.0 kHz Unknown"]
[{"$nulls":3},"09","176.4 kHz Unknown"]
[{"$nulls":3},"0A","192.0 kHz Unknown"]
[{"$nulls":3},"0B","48kHz (96kHz)"]
[null,12,"EX/EX","00","Off"]
[{"$nulls":3},"01","Matrix On"]
[{"$nulls":3},"02","Discrete ON"]
[null,13,"Thr / Bypass","00","Off"]
[{"$nulls":3},"01","On"]
[null,14,"RED dts","00","Release"]
[{"$nulls":3},"01","Wait"]
[null,15,"Tuner tuned","00","Not tuned"]
[{"$nulls":3},"01","Tuned"]
[null,16,"Dts 96/24","00","Off"]
[{"$nulls":3},"01","On"]
[null,"20","Power","00","ALL(Main/Zone2/3) OFF "]
[{"$nulls":3},"01","ALL(Main/Zone2/3) ON "]
[{"$nulls":3},"02","MainON / Zone2 OFF / Zone3 OFF "]
[{"$nulls":3},"03","03 MainOFF / Zone2 ON / Zone3 ON "]
[null,"",null,"04","MainON / Zone2 ON / Zone3 OFF "]
[null,"",null,"05","MainON / Zone2 OFF / Zone3 OFF "]
[null,"",null,"06","MainOFF / Zone2 ON / Zone3 ON "]
[null,"",null,"07","MainOFF / Zone2 OFF / Zone3 ON "]
[null,"21","Input (6 Ch Off)","00","PHONO "]
[{"$nulls":3},"01","CD "]
[null,"",null,"02","TUNER "]
[null,"",null,"03","CD-R "]
[null,"",null,"04","MD/TAPE "]
[null,"",null,"05","DVD "]
[null,"",null,"06","D-TV/LD "]
[null,"",null,"07","CBL/SAT "]
[null,"",null,"08","SAT "]
[null,"",null,"09","VCR1 "]
[null,"",null,"0A","VCR2/DVR "]
[null,"",null,"0B","VCR3/DVR "]
[null,"",null,"0C","V-AUX "]
[null,"21","Input (6 Ch Off)",10,"PHONO "]
[{"$nulls":3},11,"CD "]
[null,"",null,12,"TUNER "]
[null,"",null,13,"CD-R "]
[null,"",null,14,"MD/TAPE "]
[null,"",null,15,"DVD "]
[null,"",null,16,"D-TV/LD "]
[null,"",null,17,"CBL/SAT "]
[null,"",null,18,"SAT "]
[null,"",null,19,"VCR1 "]
[null,"",null,"1A","VCR2/DVR "]
[null,"",null,"1B","VCR3/DVR "]
[null,"",null,"1C","V-AUX "]
[null,"22","Input mode","00","AUTO "]
[{"$nulls":3},"02","DTS "]
[{"$nulls":3},"04","ANALOG "]
[{"$nulls":3},"05","ANALOG ONLY "]
[{"$nulls":3},"06","AAC "]
[null,"23","Mute","00","OFF "]
[{"$nulls":3},"01","ON "]
[null,"24","Zone 2 Input","00","PHONO "]
[{"$nulls":3},"01","CD "]
[{"$nulls":3},"02","TUNER "]
[{"$nulls":3},"03","CD-R "]
[{"$nulls":3},"04","MD/TAPE "]
[{"$nulls":3},"05","DVD 33 Neo: "]
[{"$nulls":3},"06","D-TV/LD "]
[{"$nulls":3},"07","CBL/SAT "]
[{"$nulls":3},"08","SAT "]
[{"$nulls":3},"09","VCR1 "]
[{"$nulls":3},"0A","VCR2/DVR "]
[{"$nulls":3},"0B","VCR3/DVR "]
[{"$nulls":3},"0C","V-AUX "]
[null,"25","Zone 2 Mute","00","OFF"]
[{"$nulls":3},"01","ON "]
[null,"26","Master Vol","00","-oo"]
[{"$nulls":3},"39","-80dB "]
[{"$nulls":3},"C7","0dB "]
[{"$nulls":3},"E8","16.5dB "]
[null,"27","Zone 2 Vol","00","-oo"]
[{"$nulls":3},"39","-80dB "]
[{"$nulls":3},"C7","0dB "]
[{"$nulls":3},"E8","16.5dB "]
[null,28,"Program 7 Channel","00","Hall A (HALL1)"]
[{"$nulls":3},"01","Hall B"]
[{"$nulls":3},"02","Hall C"]
[{"$nulls":3},"04","Hall C"]
[{"$nulls":3},"05","Hall E"]
[{"$nulls":3},"06","Live Concert"]
[{"$nulls":3},"08","Tokyo"]
[{"$nulls":3},"09","Freiburg"]
[{"$nulls":3},"0A","Royaumont"]
[{"$nulls":3},"0C","Village Gate"]
[{"$nulls":3},"0D","Village Vanguard"]
[{"$nulls":3},"0E","The Bottom Line"]
[{"$nulls":3},"10","The Roxy Theater"]
[{"$nulls":3},"11","Warehouse Loft"]
[{"$nulls":3},"12","Arena"]
[{"$nulls":3},"14","Disco"]
[{"$nulls":3},"15","Party"]
[{"$nulls":3},"16","Game"]
[{"$nulls":3},"17","6/8CH Stereo"]
[{"$nulls":3},"18","Pop/Rock"]
[{"$nulls":3},"19","DJ"]
[{"$nulls":3},"1C","Opera"]
[{"$nulls":3},"1D","Pavillion"]
[{"$nulls":3},"20","Mono Movie"]
[{"$nulls":3},"21","Variety Sports"]
[{"$nulls":3},"24","Spectacre"]
[null,"",null,"25","Sci-Fi"]
[{"$nulls":3},"28","Adventure"]
[{"$nulls":3},"29","General"]
[{"$nulls":3},"2C","Normal"]
[{"$nulls":3},"2D","Enhanced"]
[{"$nulls":3},"30","PLII Movie"]
[{"$nulls":3},"31","PLII Music"]
[{"$nulls":3},32,"Neo: 6 Movie"]
[null,"",null,"33","Neo: 6 Music"]
[{"$nulls":3},"36","THX A Cinema"]
[{"$nulls":3},"37","THX B Music"]
[{"$nulls":3},"34","STEREO A 2CH Stereo"]
[{"$nulls":3},"35","STEREO B 2CH Direct Stereo"]
[null,""]
[null,28,"Program Straight","80","STRAIGHT (HALL A)"]
[{"$nulls":3},"81","STRAIGHT (HALL B)"]
[{"$nulls":3},"82","Hall C"]
[{"$nulls":3},"84","Hall C"]
[{"$nulls":3},"85","Hall E"]
[{"$nulls":3},"86","Live Concert"]
[{"$nulls":3},"88","Tokyo"]
[{"$nulls":3},"89","Freiburg"]
[{"$nulls":3},"8A","Royaumont"]
[{"$nulls":3},"8C","Village Gate"]
[{"$nulls":3},"8D","Village Vanguard"]
[{"$nulls":3},"8E","The Bottom Line"]
[{"$nulls":3},"90","The Roxy Theater"]
[{"$nulls":3},"91","Warehouse Loft"]
[{"$nulls":3},"92","Arena"]
[{"$nulls":3},"94","Disco"]
[{"$nulls":3},"95","Party"]
[{"$nulls":3},"96","Game"]
[{"$nulls":3},"97","6/8CH Stereo"]
[{"$nulls":3},"98","Pop/Rock"]
[{"$nulls":3},"99","DJ"]
[{"$nulls":3},"9C","Opera"]
[{"$nulls":3},"9D","Pavillion"]
[{"$nulls":3},"A0","Mono Movie"]
[{"$nulls":3},"A1","Variety Sports"]
[{"$nulls":3},"A4","Spectacre"]
[null,"",null,"A5","Sci-Fi"]
[{"$nulls":3},"A8","Adventure"]
[{"$nulls":3},"A9","General"]
[{"$nulls":3},"AC","Normal"]
[{"$nulls":3},"AD","Enhanced"]
[{"$nulls":3},"B0","PLII Movie"]
[{"$nulls":3},"B1","PLII Music"]
[{"$nulls":3},"B2","Neo: 6 Movie"]
[null,"",null,"B3","Neo: 6 Music"]
[{"$nulls":3},"B6","THX A Cinema"]
[{"$nulls":3},"B7","THX B Music"]
[{"$nulls":3},"B4","STEREO A 2CH Stereo"]
[{"$nulls":3},"B5","STEREO B 2CH Direct Stereo"]
[null,29,"Tuner Page","00","A"]
[{"$nulls":3},"01","B"]
[{"$nulls":3},"02","C"]
[{"$nulls":3},"03","D"]
[{"$nulls":3},"04","E"]
[null,"2A","Tuner Preset No.","00",1]
[null,"",null,"01",2]
[null,"",null,"02",3]
[null,"",null,"03",4]
[null,"",null,"04",5]
[null,"",null,"05",6]
[null,"",null,"06",7]
[null,"",null,"07",8]
[null,"2B","OSD","00","Full"]
[{"$nulls":3},"01","Short"]
[{"$nulls":3},"02","Off"]
[null,"2C","Sleep","00",120]
[{"$nulls":3},"01",90]
[{"$nulls":3},"02",60]
[{"$nulls":3},"03",30]
[{"$nulls":3},"04","Off"]
[null,"2D","EX/ES(Key)","00","Off"]
[{"$nulls":3},"01","Matrix On"]
[{"$nulls":3},"02","Discrete On"]
[{"$nulls":3},"03","Auto"]
[null,"2E","SP Relay A","00","Off"]
[{"$nulls":3},"01","01 On"]
[null,"2F","SP Relay B","00","Off"]
[{"$nulls":3},"01","On"]
[null,"30","Home Preset","01","A"]
[{"$nulls":3},"02","B"]
[{"$nulls":3},"03","C"]
[{"$nulls":3},"04","D"]
[{"$nulls":3},"05","E"]
[{"$nulls":3},"06","F"]
[null,"31","Home Memory","01","A"]
[{"$nulls":3},"02","B"]
[{"$nulls":3},"03","C"]
[{"$nulls":3},"04","D"]
[{"$nulls":3},"05","E"]
[{"$nulls":3},"06","F"]
[null,"32","Home Vol. Preset","01","A"]
[{"$nulls":3},"02","B"]
[{"$nulls":3},"03","C"]
[{"$nulls":3},"04","D"]
[{"$nulls":3},"05","E"]
[{"$nulls":3},"06","F"]
[null,"33","Home Vol Memory","01","A"]
[{"$nulls":3},"02","B"]
[{"$nulls":3},"03","C"]
[{"$nulls":3},"04","D"]
[{"$nulls":3},"05","E"]
[{"$nulls":3},"06","F"]
[null,"34","Headphone","00","Off"]
[{"$nulls":3},"01","On"]
[null,"35","FM/AM","00","FM"]
[{"$nulls":3},"01","AM"]
[null,"36","DC1 Trigger","00","Off (Due to delay)"]
[{"$nulls":3},"01","On (Due to delay)"]
[null,"37","Home Zone 2 Vol Preset","01","A"]
[{"$nulls":3},"02","B"]
[{"$nulls":3},"03","C"]
[{"$nulls":3},"04","D"]
[{"$nulls":3},"05","E"]
[{"$nulls":3},"06","F"]
[null,"38","Home Zone 2 Vol","01","A"]
[{"$nulls":3},"02","B"]
[{"$nulls":3},"03","C"]
[{"$nulls":3},"04","D"]
[{"$nulls":3},"05","E"]
[{"$nulls":3},"06","F"]
[null,"39","Dual/Mono","00","Main"]
[{"$nulls":3},"01","Sub"]
[{"$nulls":3},"02","All"]
[null,"3A","DC1 Trigger Control","00","All Zone"]
[{"$nulls":3},"01","Zone 1"]
[{"$nulls":3},"02","Zone 2"]
[{"$nulls":3},"03","Zone 3"]
[null,"3B","DC2 Trigger Control","00","All Zone"]
[{"$nulls":3},"01","Zone 1"]
[{"$nulls":3},"02","Zone 2"]
[{"$nulls":3},"03","Zone 3"]
[null,"3C","DC2 Trigger Output","00","Off (Due to delay)"]
[{"$nulls":3},"01","On (Due to delay)"]
[null,"3D","Main Level","00","Normal"]
[{"$nulls":3},"01","-10 db"]
[null,"3E","SPB Set","00","Main"]
[{"$nulls":3},"01","Zone B"]
[null,"3F","Zone2 SP Out","00","Off"]
[{"$nulls":3},"01","On"]
[null,"40","Level Main Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"41","Level Main Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"42","Level Center","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"43","Level Rear Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"44","Level Rear Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"45","Level Surround Back Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"46","Level Surround Back Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"47","Level Front Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"48","Level Front Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"49","Level SWFR 1","00","-20dB"]
[{"$nulls":3},"01","-19.5dB"]
[{"$nulls":3},"28","0dB"]
[null,"4A","Level SWFR 2","00","-20dB"]
[{"$nulls":3},"01","-19.5dB"]
[{"$nulls":3},"28","0dB"]
[null,"50","Main L/R Balance","00","Left Max"]
[{"$nulls":3},"14","Middle"]
[{"$nulls":3},"28","Right Max"]
[null,"51","LFE Level SP","00","-20dB"]
[{"$nulls":3},"01","19dB"]
[{"$nulls":3},"14","0dB"]
[null,"52","LFE Level HP","00","-20dB"]
[{"$nulls":3},"01","19dB"]
[{"$nulls":3},"14","0dB"]
[null,"53","Audio Delay","00","0 ms"]
[{"$nulls":3},"A0","160 ms"]
[null,"54","SP Delay Center","00","0 ms"]
[{"$nulls":3},"01","0.5 ms"]
[{"$nulls":3},"0A","5 ms"]
[null,"55","SP Delay Rear CT","00","0 ms"]
[{"$nulls":3},"01","0.5 ms"]
[{"$nulls":3},"0A","5 ms"]
[null,"60","Input Mode","00","Auto"]
[{"$nulls":3},"01","Last"]
[null,"61","Dimmer","00",-4]
[{"$nulls":3},"01",-3]
[{"$nulls":3},"02",-2]
[{"$nulls":3},"03",-1]
[{"$nulls":3},"04",0]
[null,"62","OSD Shift","00",-5]
[{"$nulls":3},"01",-4]
[{"$nulls":3},"02",-3]
[{"$nulls":3},"03",-2]
[{"$nulls":3},"04",-1]
[{"$nulls":3},"05",0]
[{"$nulls":3},"06",1]
[{"$nulls":3},"07",2]
[{"$nulls":3},"08",3]
[{"$nulls":3},"09",4]
[{"$nulls":3},"0A",5]
[null,"63","Gray Back","00","Off"]
[{"$nulls":3},"01","Auto"]
[null,"64","Dynamic Range SP","00","Max"]
[{"$nulls":3},"01","Standard"]
[{"$nulls":3},"02","Min"]
[null,"65","Dynamic Range HP","00","Max"]
[{"$nulls":3},"01","Standard"]
[{"$nulls":3},"02","Min"]
[null,"66","Zone 2 Vol Out","00","Variable"]
[{"$nulls":3},"01","Fixed"]
[null,"67","Zone 2 Mode","00","Mode 1"]
[{"$nulls":3},"01","Mode 2"]
[null,"68","Mem Guard","00","Off"]
[{"$nulls":3},"01","On"]
[null,"69","Video Conversion","00","Off"]
[{"$nulls":3},"01","On"]
[null,"6A","COMP OSD","00","Off"]
[{"$nulls":3},"01","On"]
[null,"6B","Zone 3 Vol Out","00","Variable"]
[{"$nulls":3},"01","Fixed"]
[null,"70","Center SP","00","Large"]
[{"$nulls":3},"01","Small"]
[{"$nulls":3},"02","None"]
[null,"71","Main","00","Large"]
[{"$nulls":3},"01","Small"]
[null,"72","Rear LR SP","00","Large"]
[{"$nulls":3},"01","Small"]
[{"$nulls":3},"02","None"]
[null,"73","Surround Back","00","Large x 2"]
[{"$nulls":3},"01","Large x 1"]
[{"$nulls":3},"02","Small x 2"]
[{"$nulls":3},"03","Small x 1"]
[{"$nulls":3},"04","None"]
[null,"74","Front","00","Yes"]
[{"$nulls":3},"01","None"]
[null,"75","LFE Bass Out","00","SWFR"]
[{"$nulls":3},"01","Main"]
[{"$nulls":3},"02","Both"]
[null,"76","SW1","00","L-R"]
[{"$nulls":3},"01","F-R"]
[{"$nulls":3},"02","None"]
[null,"78","6ch Center","00","Center"]
[{"$nulls":3},"01","Main"]
[null,"79","6Ch SWFR","00","SWFR"]
[{"$nulls":3},"01","Main"]
[null,"7A","6Ch Surround","00","Surround"]
[{"$nulls":3},"01","Main"]
[null,"7B","Multi Ch Select","00","6 Ch"]
[{"$nulls":3},"01","8 Ch"]
[null,"7E","SW Crossover","00","40 Hz"]
[{"$nulls":3},"01","60 Hz"]
[{"$nulls":3},"02","80 Hz"]
[{"$nulls":3},"03","90 Hz"]
[{"$nulls":3},"04","100 Hz"]
[{"$nulls":3},"05","110 Hz"]
[{"$nulls":3},"06","120 Hz"]
[{"$nulls":3},"07","160 Hz"]
[{"$nulls":3},"08","200 Hz"]
[null,"80","Test","00","Off"]
[{"$nulls":3},"01","Dolby"]
[{"$nulls":3},"02","DSP"]
[null,"81","Analog Special","00","Off"]
[{"$nulls":3},"01","On (2 Ch)"]
[{"$nulls":3},"02","On (Multi Ch)"]
[null,"82","Night Mode","00","Off"]
[{"$nulls":3},"01","On"]
[null,83,"Tone","00","Bypass"]
[{"$nulls":3},"01","Treble Adjust"]
[{"$nulls":3},"02","Base Adjust"]
[null,84,"Treble Adjust","00","-6.0 dB"]
[{"$nulls":3},"01","-5.5 dB"]
[{"$nulls":3},"0C","0 dB"]
[{"$nulls":3},"18","+6.0 dB"]
[null,84,"Bass Adjust","00","-6.0 dB"]
[{"$nulls":3},"01","-5.5 dB"]
[{"$nulls":3},"0C","0 dB DEFECT - it always reports 0C, even though it changes the sound and the display updates"]
[{"$nulls":3},"18","+6.0 dB"]
[null,"90","Multi Ch Level Main Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"91","Multi Ch Level Main Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"92","Multi Ch Level Center","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"93","Multi Ch Level Rear Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"94","Multi Ch Level Rear Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"95","Multi Ch Level Surround Back Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"96","Multi Ch Level Surround Back Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"97","Multi Ch Level Front Right","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"98","Multi Ch Level Front Left","14","-10dB …"]
[{"$nulls":3},"3C","+10dB"]
[null,"99","Multi Ch Level SWFR 1","00","-20dB"]
[{"$nulls":3},"01","-19.5dB"]
[{"$nulls":3},"28","0dB"]
[null,"9A","Multi Ch Level SWFR 2","00","-20dB"]
[{"$nulls":3},"01","-19.5dB"]
[{"$nulls":3},"28","0dB"]
[]
[null,"A0","Zone 3 Input","00","PHONO "]
[{"$nulls":3},"01","CD "]
[{"$nulls":3},"02","TUNER "]
[{"$nulls":3},"03","CD-R "]
[{"$nulls":3},"04","MD/TAPE "]
[{"$nulls":3},"05","DVD "]
[{"$nulls":3},"06","D-TV/LD "]
[{"$nulls":3},"07","CBL/SAT "]
[{"$nulls":3},"08","SAT "]
[{"$nulls":3},"09","VCR1 "]
[{"$nulls":3},"0A","VCR2/DVR "]
[{"$nulls":3},"0B","VCR3/DVR "]
[{"$nulls":3},"0C","V-AUX "]
[null,"A1","Zone 3 Mute","00","OFF "]
[{"$nulls":3},"01","ON "]
[null,"A2","Zone 3 Volume","00","-oo"]
[{"$nulls":3},"39","-80dB "]
[{"$nulls":3},"C7","0dB "]
[{"$nulls":3},"E8","16.5dB "]

{"sheet":"Status Block","index":4,"n_rows":139,"n_cols":2,"rows_kept":139}
["DT Offset","Description"]
[0,"* Baud Rate '@'"]
[1,"* Receive Buffer  'E'"]
[2,"* Receive Buffer  '0'"]
[3,"*                 '1'"]
[4,"* Command Timeout '9'"]
[5,"*                 '0'"]
[6,"*                 '0'"]
[7,"* System          '0':Ok, '1':Busy"]
[8,"* Power            0:Off, 1:All On, 2:Zone1 On, 3: Zone2,3 On, 4: Zone1,2 On, 5: Zone1 On, 6: Zone2,3 On, 7: Zone3 On"]
[9,"Input      0: Phono, 1:CD, 2:Tuner, 3:CD-R, 4:MD-Tape, 5:DVD, 6:D-TV, 7:Cbl, 9:VCR1, A:VCR2"]
[10,"6ch input 0:Off, 1:On"]
[11,"Input Mode 0:AUTO, 2:DTS, 4:Analog, 5:Analog Only"]
[12,"Audio Mute 0:Off, 1:On"]
[13,"Zone2 Input 0: PHONO / 1: CD / 2: TUNER / 3: CD-R / 4: MD-TAPE / 5: DVD / 6: D-TV-LD / 7: CBL-SAT / 9: VCR1 / A: VCR2-DVR / C: V-AUX"]
[14,"Zone2 Mute 0: OFF / 1: ON"]
[15,"Master Volume Upper 4 bit"]
[16,"Master Volume Lower 4 bit"]
[17,"Zone2 Volume Upper 4 bit"]
[18,"Zone2 Volume Lower 4 bit"]
[19,"Program Upper 4 bit"]
[20,"Program Lower 4 bit"]
[21,"Effect 0: OFF / 1: ON"]
[22,"6.1/ES key status 0: OFF / 1: MATRIX ON / 2: DISCRETE ON / 3: AUTO"]
[23,"OSD* 0: FULL / 1: SHORT / 2: OFF"]
[24,"Sleep 0: 120 / 2: 90 / 3: 60 / 4: 30 / 5: OFF"]
[25,"Tuner Page 0: Page A / 1: Page B / 2: Page C / 3: Page D / 4: PageE"]
[26,"Tuner No. 0: No.1 / 1: No.2 / 2: No.3 / 3: No.4 / 4: No.5 / 5: No.6 / 6: No.7 / 7: No.8"]
[27,"Night mode 0: OFF / 1: ON"]
[28,"Care"]
[29,"Speaker relay A 0: OFF / 1: ON"]
[30,"Speaker relay B 0: OFF / 1: ON"]
[31,"Playback 0: 6ch input / 1: Analog / 2: PCM / 3: DD*(except 2.0) / 4: DD(2.0) / 5: DD.Karaoke / 6: DD.EX / 7: DTS / 8: DTS-ES / 9: Other DIGITAL / A: DTS Analog Mute / B: DTS ES Discrete"]
[32,"Fs 0: Analog / 1: 32kHz / 2: 44.1kHz / 3: 48kiHz / 4: 64kHz / 5: 88.2kHz / 6: 96kHz / 7: Unknown B: DTS 96/24"]
[33,"EX/ES playback 0: OFF / 1: MATRIX ON / 2: DISCRETE ON"]
[34,"Thr / Bypass 0: Normal / 1: Bypass"]
[35,"RED dts 0: Release / 1: Wait"]
[36,"Head Phone 0: OFF / 1: ON"]
[37,"TUNER BAND 0: FM / 1: AM"]
[38,"TUNER TUNED 0: NOT TUNED / 1: TUNED"]
[39,"DC1 Control Out 0: LOW / 1: HIGH"]
[40,"Don’t care"]
[41,"Don't Care"]
[42,"0-2 DC1 TRG Ctrl. 0: Zone1 / 1: Zone2 / 2: Zone1&2"]
[43,"0/1 dts 96/24 0: OFF / 1: ON"]
[44,"0-2 DC2 TRG Ctrl. 0: Zone1 / 1: Zone2 / 2: Zone1&2"]
[45,"0/1 DC2 Trigger 0: LOW / 1: HIGH"]
[46,"SP B set 0: Zone1 / 1: Zone2"]
[47,"Zone 2 SP out 0: OFF / 1: ON"]
[48,"MAIN R Upper 4bit"]
[49,"Lower 4bit"]
[50,"MAIN L Upper 4bit"]
[51,"Main L Lower 4bit"]
[52,"CENTER Upper 4bit"]
[53,"Center Lower 4bit"]
[54,"REAR R Upper 4bit"]
[55,"REAR R Lower 4bit"]
[56,"REAR L Upper 4bit"]
[57,"REAR L Lower 4bit"]
[58,"SUR BACK R Upper 4bit"]
[59,"SUR BACK R Lower 4bit"]
[60,"SUR BACK L Upper 4bit"]
[61,"SUR BACK L Lower 4bit"]
[62,"FRONT R Upper 4bit"]
[63,"FRONT R Lower 4bit"]
[64,"FRONT L Upper 4bit"]
[65,"FRONT L Lower 4bit"]
[66,"SWFR 1 Upper 4bit"]
[67,"SWFR 1 Lower 4bit"]
[68,"Don't Care"]
[69,"Don't Care"]
[70,"Don't Care"]
[71,"Don't Care"]
[72,"Don't Care"]
[73,"Don't Care"]
[74,"LFE Lvl. SP Upper 4bit"]
[75,"LFE Lvl. SP Lower 4bit"]
[76,"LFE Lvl. HP Upper 4bit"]
[77,"LFE Lvl. HP Lower 4bit"]
[78,"Audio Delay Upper 4bit"]
[79,"Audio Delay Lower 4bit"]
[80,"Don't Care"]
[81,"Don't Care"]
[82,"Don't Care"]
[83,"Don't Care"]
[84,"Input mode set 0: AUTO / 1: LAST"]
[85,"Dimmer 0: -4 / 1: -3 / 2: -2 / 3: -1 / 4: 0"]
[86,"OSD Message"]
[87,"OSD shift Upper 4bit"]
[88,"OSD shift Lower 4bit"]
[89,"Glay back 0: OFF / 1: AUTO"]
[90,"Video conversion 0: OFF / 1: ON"]
[91,"D. Range SP 0: MAX / 1: STD / 2: MIN"]
[92,"HP 0: MAX / 1: STD / 2: MIN"]
[93,"Zone 2 vol. Out"]
[94,"Don't Care"]
[95,"Memory guard 0: OFF / 1: ON"]
[96,"SP set Center 0: Large / 1: Small / 2: None"]
[97,"Main 0: Large / 1: Small"]
[98,"Rear L/R 0: Large / 1: Small / 2: None"]
[99,"Rear CT 0: Large / 1: Small / 2: None"]
[100,"Front 0: Yes / 1: None"]
[101,"LFE/BASS 0: SWFR / 1: Main / 2: Both"]
[102,"6CH Center 0: Center / 1: Main"]
[103,"SWFR 0: SWFR / 1: Main"]
[104,"Main level 0: Normal / 1: -10dB"]
[105,"Test mode 0: OFF / 1: Dolby / 2: DTS"]
[106,"Don't Care"]
[107,"LVL 6CH MAIN L Upper 4bit"]
[108,"LVL 6CH MAIN L Lower 4bit"]
[109,"MAIN R Upper 4bit"]
[110,"MAIN R Lower 4bit"]
[111,"CENTER Upper 4bit"]
[112,"CENTER Lower 4bit"]
[113,"SL Upper 4bit"]
[114,"SL Lower 4bit"]
[115,"SR Upper 4bit"]
[116,"SR Lower 4bit"]
[117,"SBL Upper 4bit"]
[118,"SBL Lower 4bit"]
[119,"SBR Upper 4bit"]
[120,"SBR Lower 4bit"]
[121,"FRONT L Upper 4bit"]
[122,"FRONT L Lower 4bit"]
[123,"FRONT R Upper 4bit"]
[124,"FRONT R Lower 4bit"]
[125,"SWFR Upper 4bit"]
[126,"SWFR Lower 4bit"]
[127,"0 - C Z3 Input"]
[128,"0/1 Z3 Mute"]
[129,"0 - F Z3 Volume Upper 4bit"]
[130,"0 - F Z3 Volume Lower 4bit"]
[131,"Don't Care"]
[132,"MULTI_CH SELECT 00:6CH / 01:8CH TUNER / 02: 8CH CD / 04: 8CH CD-R / 05: 8CH DVD / 06: DTV / 07: 8CH CBL/SAT / 09: 8CH VCR1 / 0A: VCR2/DVR / 0C: VAUX"]
[133,"MULTI_CH SURROUND to 00: Surround / 01: Main"]
[134,"SP SET SW1 00: L-R / 01: F-R / 02: NONE"]
[135,"SP SET CROSSOVER 00: 40Hz / 01: 60Hz / 02: 80Hz / 03: 90Hz / 04: 100Hz / 05: 110Hz / 06: 120Hz / 07: 160Hz / 08: 200Hz"]
[136,"COMPONENT OSD 00: OFF / 01: ON"]
[137,"PB/SB SELECT 00: PR / 01: SB"]