<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<hole x="-37.3126" y="66.04" drill="2.8"/>
<hole x="-1.905" y="66.04" drill="2.8"/>
<hole x="4.191" y="81.026" drill="2.8"/>
<hole x="31.369" y="80.772" drill="2.8"/>
<hole x="-38.862" y="91.948" drill="3.2"/>
<hole x="38.862" y="91.694" drill="3.2"/>
<hole x="39.116" y="26.67" drill="3.2"/>
<hole x="-38.862" y="26.67" drill="3.2"/>
<text>Tie Strap</text>
<text>Tie Strap</text>
<text>Designed by Smartware Computing</text>
<text>Hughes Fire Equipment, Inc.</text>
<text>C:/Projects/HughesTelematic/Hardware/HFE_Logo.bmp</text>
<text>Hughes Fire 
Equipment, Inc.</text>
</plain>
<libraries>
<library name="Enclosures-PCBs">
<packages>
<package name="DTM13-12P-12P">
<description>&lt;b&gt;PCB for TE DTM13-12P*-12P#-R008&lt;/b&gt;&lt;br/&gt;
TE - Deutsch Enclosure for dual connectors (gray and black)</description>
</package>
</packages>
</library>
<library name="Smartware">
<description>&lt;b&gt;Various custom created components&lt;/b&gt;&lt;p&gt;
which may or may not have use elsewhere.</description>
<packages>
<package name="XBEE-PRO">
<description>&lt;b&gt;XBEE Pro&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
<package name="SO8">
<description>&lt;B&gt;SO8: plastic small outline package; 8 leads; body width 3.9 mm&lt;/B&gt;&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/PCA82C250.pdf</description>
</package>
<package name="MOLEX-SD-503182-005">
<description>&lt;b&gt;Molex Micro SD&lt;/b&gt;&lt;br/&gt;
Part Number: SD-503182-005
Top mount&lt;br/&gt;
Push-in, Push-out&lt;br/&gt;
Source: &lt;a href="http://www.digikey.com/product-detail/en/5031820832/WM6873CT-ND/3045274"&gt;DigiKey&lt;/a&gt;</description>
</package>
<package name="JP-3PIN-SMALL-PAD">
<description>&lt;b&gt;JUMPER - 3-pin with all small pads&lt;/b&gt;&lt;br/&gt;
Where routing requires small pads</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="1X02">
</package>
<package name="TP-031">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="QSOP16">
<description>&lt;b&gt;16-Lead Shrink Small Outline Package&lt;/b&gt; QSOP (RQ-16)&lt;p&gt;
Source: ADG658_659.pdf</description>
</package>
<package name="DDC0006A_N">
</package>
<package name="SMA">
</package>
<package name="SRN6045">
</package>
<package name="SRU8043">
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="DR331-513AE">
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SOD123">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="tran-bjt">
<description>&lt;strong&gt;&lt;big&gt;&lt;u&gt;Bipolar Junction Transistor (BJT) Device Library&lt;/u&gt;&lt;/big&gt;&lt;/strong&gt;
&lt;p&gt;
&lt;strong&gt;Wildwood Electronics Specialists Standard Library for Eagle (WESSLE)&lt;/strong&gt;&lt;br&gt;&lt;author&gt;martin@wild-wood.net&lt;/author&gt;

&lt;p&gt;Small-signal and power NPN and PNP BJTs and IGBTs</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="passive">
<description>&lt;strong&gt;&lt;big&gt;&lt;u&gt;Passive Device Library&lt;/u&gt;&lt;/big&gt;&lt;/strong&gt;
&lt;p&gt;
&lt;strong&gt;Wildwood Electronics Specialists Standard Library for Eagle (WESSLE)&lt;/strong&gt;&lt;br&gt;&lt;author&gt;martin@wild-wood.net&lt;/author&gt;
&lt;p&gt;
Resistors, varistors, thermistors, trimmers/potentiomerers, resistor arrays
&lt;br&gt;Capacitors (non-polar and polar), capacitor arrays
&lt;br&gt; inductors, ferrite beads, common-mode chokes
&lt;br&gt;General impedance
&lt;p&gt;&lt;font color=blue&gt;This library makes extensive use of &lt;u&gt;automatic part number generation&lt;/u&gt; using the ULP "&lt;em&gt;wwes_bom.ulp&lt;/em&gt;". For thick-film chip resistors, thick-film chip resistor arrays, multi-layer ceramic chip (MLCC) capacitors, MLCC capacitor arrays, aluminum electrolytic capacitors, and tantalum capacitors, the component value is specified (and optional tolerance, voltage rating, etc) and a part number is generated for the component in the BOM. Please refer to the documentation for "&lt;em&gt;wwes_bom.ulp&lt;/em&gt;" for more information.&lt;/font&gt;</description>
<packages>
<package name="1206">
<description>1206 SMT chip</description>
</package>
<package name="SRF0905">
<description>Bourns SRF0905 Series Line Filter / Common-Mode Choke Package</description>
</package>
<package name="1210">
<description>1210 SMT chip</description>
</package>
<package name="0805">
<description>0805 SMT chip</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mbed-microcontroller">
<packages>
<package name="MBED-SOCKET-DUALROW">
<description>&lt;b&gt;Dual Row Socket&lt;/b&gt;&lt;br/&gt;
For an mbed LPC1768 module.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Enclosures-PCBs" package="DTM13-12P-12P" value="DTM13-12PA-12PB-R008"/>
<element name="MOD2" library="Smartware" package="XBEE-PRO" value="XBEE-PRO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="Smartware" package="SO08" value="BTS4175SGA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="Smartware" package="SO08" value="BTS4175SGA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="Smartware" package="SO08" value="BTS4175SGA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="Smartware" package="SO08" value="BTS4175SGA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="Smartware" package="SO8" value="SN65HVD252D">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1085275"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="Smartware" package="SO8" value="SN65HVD252D">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1085275"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="Smartware" package="SOIC8" value="DS36277TMX/NOPB">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON1" library="Smartware" package="MOLEX-SD-503182-005" value="MICROSD">
<attribute name="FEATURES" value="Push-Pull"/>
<attribute name="MPN" value="5031821852"/>
<attribute name="OC_DIGIKEY" value="WM12834CT-ND"/>
<attribute name="MF" value="Molex"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="49.9K 1% - RNCP0805FTD49K9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0805" value="13.3K 1% - ERJ-6ENF1332V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MF" value="Diodes Inc"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0805" value="20.0K 1% - RNCP0805FTD20K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="39.2K 1% - RNCP0805FTD39K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MF" value="Diodes Inc"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="20.0K 1% - RNCP0805FTD20K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="39.2K 1% - RNCP0805FTD39K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D14" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MF" value="Diodes Inc"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0805" value="20.0K 1% - RNCP0805FTD20K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0805" value="39.2K 1% - RNCP0805FTD39K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D15" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MF" value="Diodes Inc"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="R0805" value="20.0K 1% - RNCP0805FTD20K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="R0805" value="39.2K 1% - RNCP0805FTD39K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D16" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MF" value="Diodes Inc"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="47R 1% 0.5W - CRCW080547R0JNEAHP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="47R 1% 0.5W - CRCW080547R0JNEAHP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="Smartware" package="C0805" value="0.022uF 50V - C0805C223K5RACTU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="Smartware" package="C0805" value="0.022uF 50V - C0805C223K5RACTU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="4.7K 1% - RMCF0805FT4K70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="4.7K 1% - RMCF0805FT4K70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="Smartware" package="C0805" value="1uF 16v - EMK212BJ105KGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="Smartware" package="C0805" value="1uF 16v - EMK212BJ105KGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="Smartware" package="C0805" value="1uF 16v - EMK212BJ105KGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="Smartware" package="1X02" value="2PIN - M20-9990246">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Smartware" package="1X02" value="2PIN - M20-9990246">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0805" value="15K 1% - RNCP0805FTD15K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0805" value="6.8k 0.25W - ERJ-PB6D6801V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MF" value="Diodes Inc"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MF" value="Diodes Inc"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MF" value="Diodes Inc"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="10K 1% - RMCF0805FT10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MF" value="Diodes Inc"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R0805" value="6.8k 0.25W - ERJ-PB6D6801V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0805" value="6.8k 0.25W - ERJ-PB6D6801V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="6.8k 0.25W - ERJ-PB6D6801V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="Smartware" package="JP-3PIN-SMALL-PAD" value="3PIN_VPAD - 61300311121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP21" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP20" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP19" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP18" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP17" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP16" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP23" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP24" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP25" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP26" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP27" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP28" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP29" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP30" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP31" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP41" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP40" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP39" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP38" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP37" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP36" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP35" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP34" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP33" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP32" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP22" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="U11" library="Smartware" package="SO08" value="TS2951CS50 RLG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP5" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP6" library="Smartware" package="TP-031" value="TEST_PAD_IL-031"/>
<element name="TP3" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="Smartware" package="TP-031" value="TEST_PAD_IL-031">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="Smartware" package="QSOP16" value="ADM3101EARQZ-REEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="Smartware" package="C0805" value="1uF 16v - EMK212BJ105KGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="Smartware" package="C0805" value="1uF 16v - EMK212BJ105KGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="Smartware" package="DDC0006A_N" value="LMR14010ADDCR">
<attribute name="PARTNUMBER" value="LMR14010ADDCR"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LMR14010ADDCR"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="TYPE" value="TYPE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="Smartware" package="DDC0006A_N" value="LMR14010ADDCR">
<attribute name="PARTNUMBER" value="LMR14010ADDCR"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LMR14010ADDCR"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="TYPE" value="TYPE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="Smartware" package="SMA" value="60V 2A - SS26FL">
<attribute name="IO" value="2.0"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SK220ATR"/>
<attribute name="VFATIO" value="0.9"/>
<attribute name="DATASHEETURL" value="httpwww.smc%2Ddiodes.compropdfSK220A%2520N0942%2520REV.A.pdf"/>
<attribute name="VRRM" value="200.0"/>
<attribute name="VENDOR" value="SMC Diode Solutions"/>
<attribute name="MANUFACTURER_NAME" value="SMC Diode Solutions"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Smartware" package="SRN6045" value="33uH 1.4A 100mR - SRU8043-330Y">
<attribute name="MANUFACTURER_PART_NUMBER" value="SRN6045150M"/>
<attribute name="L" value="1.5E5"/>
<attribute name="DATASHEETURL" value="httpwww.bourns.comdataglobalpdfsSRN6045.pdf"/>
<attribute name="IDC" value="1.9"/>
<attribute name="DCR" value="0.0958"/>
<attribute name="VENDOR" value="Bourns"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Smartware" package="SRU8043" value="15uH 1.9A 95.8mR - SRN6045-150M">
<attribute name="MANUFACTURER_PART_NUMBER" value="SRU8043330Y"/>
<attribute name="L" value="3.3E5"/>
<attribute name="IDC" value="1.7"/>
<attribute name="DCR" value="0.1"/>
<attribute name="VENDOR" value="Bourns"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Smartware" package="R0805" value="20k 1% - CRCW080520K0FKEA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Smartware" package="R0805" value="111K 0.1% - PTN0805E1113BST1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Smartware" package="C0603" value="1uF 50V - C1608X5R1H105K080AB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Smartware" package="C0603" value="1uF 50V - C1608X5R1H105K080AB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Smartware" package="C0603" value="1uF 50V - C1608X5R1H105K080AB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="Smartware" package="C0603" value="1uF 50V - C1608X5R1H105K080AB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="Smartware" package="C1206" value="10uF 25V - CL31A106KAHNNNE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="Smartware" package="C1206" value="10uF 25V - CL31A106KAHNNNE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="Smartware" package="C1206" value="22uF 16V - C2012X6S1C226M125AC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="Smartware" package="C1206" value="22uF 16V - C2012X6S1C226M125AC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Smartware" package="C0805" value="100nF 50V - C0805C104M5RACTU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Smartware" package="C0805" value="100nF 50V - C0805C104M5RACTU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="10k 1% - RNCF0805DTE10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="16.9k 1% - RNCF0805DTE16K9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="Smartware" package="C0805" value="1uF 10V - 0805ZC105KAT2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="249K 1% - RMCF0805FT249K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="Smartware" package="C0805" value="0.1uF 10v - 0805ZD104KAT2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="Smartware" package="C0805" value="0.1uF 10v - 0805ZD104KAT2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="Smartware" package="C0805" value="0.1uF 10v - 0805ZD104KAT2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="Smartware" package="SOT23" value="24V TVS - NUP2105LT1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="Smartware" package="SOT23" value="24V TVS - NUP2105LT1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="Smartware" package="DR331-513AE" value="51uH 500mA - Bourns DR331-513AE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="Smartware" package="DR331-513AE" value="51uH 500mA - Bourns DR331-513AE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="Smartware" package="SMA" value="60V 2A - SS26FL">
<attribute name="MANUFACTURER_PART_NUMBER" value="SK220ATR"/>
<attribute name="DATASHEETURL" value="httpwww.smc%2Ddiodes.compropdfSK220A%2520N0942%2520REV.A.pdf"/>
<attribute name="VRRM" value="200.0"/>
<attribute name="MANUFACTURER_NAME" value="SMC Diode Solutions"/>
<attribute name="VFATIO" value="0.9"/>
<attribute name="IO" value="2.0"/>
<attribute name="VENDOR" value="SMC Diode Solutions"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Smartware" package="R0805" value="64.9k 1% - CRCW080564K9FKEA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Smartware" package="R0805" value="19.6k 1% - ERJ-6ENF1962V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Smartware" package="SOT23" value="BAS40-04-7-F">
<attribute name="OC_DIGIKEY" value="BAS40-04FDICT-ND"/>
<attribute name="MF" value="Diodes Inc"/>
<attribute name="MPN" value="BAS40-04-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Smartware" package="SOT23" value="BSS123LT1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Smartware" package="SOT23" value="BSS123LT1G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Smartware" package="C0805" value="100nF 6.3V -  C0805C104K9RACTU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="tran-bjt" package="SOT223" value="FZT653TA">
<attribute name="MFG" value="Diodes Inc."/>
<attribute name="DIGIKEY" value="FZT653CT-ND"/>
<attribute name="VCE" value="100v"/>
<attribute name="IC" value="2A"/>
<attribute name="VCESAT" value="500mV"/>
<attribute name="DESC" value="100V NPN (SOT223)"/>
<attribute name="PMAX" value="2W"/>
<attribute name="NAME"/>
</element>
<element name="D3" library="Smartware" package="SOT23" value="MMBZ5254BLT1">
<attribute name="NAME"/>
</element>
<element name="R3" library="passive" package="1206" value="1.5k 1% - RNCP0805FTD1K50">
<attribute name="PWR" value="250mW"/>
<attribute name="TYPE" value="RES"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="passive" package="SRF0905" value="SRF0905-501Y">
<attribute name="MFG" value="Bourns"/>
<attribute name="DCR" value="0.15"/>
<attribute name="IRATED" value="1.0A"/>
<attribute name="VRATED" value="80V"/>
<attribute name="L" value="500uH"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="passive" package="0805" value="100n 100V - C2012X7R2A104K125AA">
<attribute name="TYPE" value="CAP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="passive" package="0805" value="100n 100V - C2012X7R2A104K125AA">
<attribute name="TYPE" value="CAP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="passive" package="PANASONIC_D" value="100u 35V - EEH-ZK1V101XP">
<attribute name="TYPE" value="CELE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="passive" package="PANASONIC_D" value="100u 35V - EEH-ZK1V101XP">
<attribute name="TYPE" value="CELE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="passive" package="1210" value="0.47uF 50V - 50MU474MB13225">
<attribute name="TYPE" value="CAP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="passive" package="1210" value="0.47uF 50V - 50MU474MB13225">
<attribute name="TYPE" value="CAP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOD1" library="mbed-microcontroller" package="MBED-SOCKET-DUALROW" value="MBED-MODULEDUAL - LPC1768">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Smartware" package="SOD123" value="60V 2A - MBR130T1G">
<attribute name="OC_DK" value="MBR130T1GOSCT-ND"/>
<attribute name="MF" value="On Semi"/>
<attribute name="MFN" value="MBR130T1G"/>
</element>
</elements>
<signals>
<signal name="0V0">
<contactref element="U7" pad="1"/>
<contactref element="U9" pad="1"/>
<contactref element="U10" pad="1"/>
<contactref element="U8" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="D13" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="D14" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="D15" pad="1"/>
<contactref element="R39" pad="1"/>
<contactref element="D16" pad="1"/>
<contactref element="J8" pad="3"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="D9" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="D10" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="D11" pad="1"/>
<contactref element="D12" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="J9" pad="3"/>
<contactref element="J10" pad="3"/>
<contactref element="J11" pad="3"/>
<contactref element="J1" pad="J-G4"/>
<contactref element="J1" pad="J-G3"/>
<contactref element="R8" pad="1"/>
<contactref element="U4" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U11" pad="4"/>
<contactref element="C12" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="TP2" pad="TP"/>
<contactref element="C3" pad="2"/>
<contactref element="T1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="D3" pad="1"/>
<contactref element="C6" pad="-"/>
<contactref element="C9" pad="-"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="CON1" pad="M1"/>
<contactref element="CON1" pad="M2"/>
<contactref element="CON1" pad="M3"/>
<contactref element="CON1" pad="M4"/>
<contactref element="CON1" pad="6"/>
<contactref element="MOD2" pad="10"/>
<contactref element="TP31" pad="TP"/>
<contactref element="C20" pad="2"/>
<contactref element="C22" pad="1"/>
<contactref element="U5" pad="9"/>
<contactref element="IC2" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="D7" pad="3"/>
<contactref element="U6" pad="5"/>
<contactref element="C26" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="U6" pad="4"/>
<contactref element="U6" pad="2"/>
<contactref element="MOD1" pad="P$1"/>
<contactref element="MOD1" pad="P$41"/>
</signal>
<signal name="GPIO1">
<contactref element="U7" pad="3"/>
<contactref element="R34" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="J1" pad="J-B4"/>
</signal>
<signal name="GPIO2">
<contactref element="U8" pad="3"/>
<contactref element="R20" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="J1" pad="J-B3"/>
</signal>
<signal name="GPIO3">
<contactref element="U9" pad="3"/>
<contactref element="R21" pad="1"/>
<contactref element="R36" pad="2"/>
<contactref element="J1" pad="J-B6"/>
</signal>
<signal name="GPIO4">
<contactref element="U10" pad="3"/>
<contactref element="R22" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="J1" pad="J-B5"/>
</signal>
<signal name="SENSOR_5V0">
<contactref element="U11" pad="1"/>
<contactref element="U11" pad="2"/>
<contactref element="J1" pad="J-G9"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="RS-485_A">
<contactref element="R11" pad="1"/>
<contactref element="J1" pad="J-B8"/>
</signal>
<signal name="RS-485_B">
<contactref element="R12" pad="1"/>
<contactref element="J1" pad="J-B7"/>
</signal>
<signal name="5V0">
<contactref element="U6" pad="8"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC3" pad="3"/>
<contactref element="R10" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="MOD1" pad="P$2"/>
<contactref element="MOD1" pad="P$42"/>
</signal>
<signal name="RS232_TX">
<contactref element="U5" pad="12"/>
<contactref element="J1" pad="J-B12"/>
</signal>
<signal name="RS232_RX">
<contactref element="U5" pad="13"/>
<contactref element="J1" pad="J-B11"/>
</signal>
<signal name="CAN2_L">
<contactref element="L3" pad="1"/>
<contactref element="J1" pad="J-G2"/>
</signal>
<signal name="CAN2_H">
<contactref element="L3" pad="2"/>
<contactref element="J1" pad="J-G1"/>
</signal>
<signal name="CAN1_L">
<contactref element="L4" pad="1"/>
<contactref element="J1" pad="J-G10"/>
</signal>
<signal name="CAN1_H">
<contactref element="L4" pad="2"/>
<contactref element="J1" pad="J-G11"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="4"/>
<contactref element="MOD1" pad="P$30"/>
<contactref element="MOD1" pad="P$70"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="1"/>
<contactref element="MOD1" pad="P$29"/>
<contactref element="MOD1" pad="P$69"/>
</signal>
<signal name="N$17">
<contactref element="IC3" pad="4"/>
<contactref element="MOD1" pad="P$9"/>
<contactref element="MOD1" pad="P$49"/>
</signal>
<signal name="N$18">
<contactref element="IC3" pad="1"/>
<contactref element="MOD1" pad="P$50"/>
<contactref element="MOD1" pad="P$10"/>
</signal>
<signal name="N$19">
<contactref element="MOD2" pad="3"/>
<contactref element="TP24" pad="TP"/>
<contactref element="MOD1" pad="P$28"/>
<contactref element="MOD1" pad="P$68"/>
</signal>
<signal name="N$20">
<contactref element="MOD2" pad="2"/>
<contactref element="TP23" pad="TP"/>
<contactref element="MOD1" pad="P$67"/>
<contactref element="MOD1" pad="P$27"/>
</signal>
<signal name="N$21">
<contactref element="MOD2" pad="4"/>
<contactref element="TP25" pad="TP"/>
<contactref element="MOD1" pad="P$26"/>
<contactref element="MOD1" pad="P$66"/>
</signal>
<signal name="N$22">
<contactref element="MOD2" pad="15"/>
<contactref element="TP37" pad="TP"/>
<contactref element="MOD1" pad="P$25"/>
<contactref element="MOD1" pad="P$65"/>
</signal>
<signal name="NC_39">
<contactref element="TP13" pad="TP"/>
<contactref element="MOD1" pad="P$39"/>
<contactref element="MOD1" pad="P$79"/>
</signal>
<signal name="EXT_3V3">
<contactref element="TP12" pad="TP"/>
<contactref element="CON1" pad="4"/>
<contactref element="MOD1" pad="P$40"/>
<contactref element="MOD1" pad="P$80"/>
</signal>
<signal name="NC_38">
<contactref element="TP14" pad="TP"/>
<contactref element="MOD1" pad="P$78"/>
<contactref element="MOD1" pad="P$38"/>
</signal>
<signal name="NC_37">
<contactref element="TP15" pad="TP"/>
<contactref element="MOD1" pad="P$77"/>
<contactref element="MOD1" pad="P$37"/>
</signal>
<signal name="NC_36">
<contactref element="TP16" pad="TP"/>
<contactref element="MOD1" pad="P$36"/>
<contactref element="MOD1" pad="P$76"/>
</signal>
<signal name="NC_35">
<contactref element="TP17" pad="TP"/>
<contactref element="MOD1" pad="P$35"/>
<contactref element="MOD1" pad="P$75"/>
</signal>
<signal name="NC_34">
<contactref element="TP18" pad="TP"/>
<contactref element="MOD1" pad="P$34"/>
<contactref element="MOD1" pad="P$74"/>
</signal>
<signal name="NC_33">
<contactref element="TP19" pad="TP"/>
<contactref element="MOD1" pad="P$73"/>
<contactref element="MOD1" pad="P$33"/>
</signal>
<signal name="NC_32">
<contactref element="TP20" pad="TP"/>
<contactref element="MOD1" pad="P$72"/>
<contactref element="MOD1" pad="P$32"/>
</signal>
<signal name="NC_31">
<contactref element="TP21" pad="TP"/>
<contactref element="MOD1" pad="P$31"/>
<contactref element="MOD1" pad="P$71"/>
</signal>
<signal name="RTC_BAT">
<contactref element="TP10" pad="TP"/>
<contactref element="MOD1" pad="P$43"/>
<contactref element="MOD1" pad="P$3"/>
</signal>
<signal name="3V3">
<contactref element="MOD2" pad="1"/>
<contactref element="D8" pad="2"/>
<contactref element="D13" pad="2"/>
<contactref element="D14" pad="2"/>
<contactref element="D15" pad="2"/>
<contactref element="D16" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="D11" pad="2"/>
<contactref element="D12" pad="2"/>
<contactref element="TP22" pad="TP"/>
<contactref element="L2" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="CON1" pad="3"/>
<contactref element="MOD1" pad="P$45"/>
<contactref element="MOD1" pad="P$5"/>
</signal>
<signal name="N$24">
<contactref element="CON1" pad="7"/>
<contactref element="MOD1" pad="P$6"/>
<contactref element="MOD1" pad="P$46"/>
</signal>
<signal name="N$25">
<contactref element="CON1" pad="5"/>
<contactref element="MOD1" pad="P$47"/>
<contactref element="MOD1" pad="P$7"/>
</signal>
<signal name="N$26">
<contactref element="CON1" pad="2"/>
<contactref element="MOD1" pad="P$8"/>
<contactref element="MOD1" pad="P$48"/>
</signal>
<signal name="NC_S1">
<contactref element="CON1" pad="S1"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="NC_S2">
<contactref element="CON1" pad="S2"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="AIN5">
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="D8" pad="3"/>
<contactref element="MOD1" pad="P$20"/>
<contactref element="MOD1" pad="P$60"/>
</signal>
<signal name="RS_A_P">
<contactref element="J2" pad="2"/>
<contactref element="MOD1" pad="P$53"/>
<contactref element="MOD1" pad="P$13"/>
</signal>
<signal name="RS_A_N">
<contactref element="J3" pad="2"/>
<contactref element="MOD1" pad="P$14"/>
<contactref element="MOD1" pad="P$54"/>
</signal>
<signal name="ASENSE1">
<contactref element="R23" pad="2"/>
<contactref element="J1" pad="J-G8"/>
</signal>
<signal name="ASENSE2">
<contactref element="R30" pad="2"/>
<contactref element="J1" pad="J-G6"/>
</signal>
<signal name="ASENSE3">
<contactref element="R32" pad="2"/>
<contactref element="J1" pad="J-G5"/>
</signal>
<signal name="ASENSE4">
<contactref element="R38" pad="2"/>
<contactref element="J1" pad="J-G7"/>
</signal>
<signal name="AIN1">
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="D13" pad="3"/>
<contactref element="MOD1" pad="P$16"/>
<contactref element="MOD1" pad="P$56"/>
</signal>
<signal name="AIN2">
<contactref element="R30" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="D14" pad="3"/>
<contactref element="MOD1" pad="P$17"/>
<contactref element="MOD1" pad="P$57"/>
</signal>
<signal name="AIN3">
<contactref element="R32" pad="1"/>
<contactref element="R33" pad="2"/>
<contactref element="D15" pad="3"/>
<contactref element="MOD1" pad="P$59"/>
<contactref element="MOD1" pad="P$19"/>
</signal>
<signal name="AIN4">
<contactref element="R38" pad="1"/>
<contactref element="R39" pad="2"/>
<contactref element="D16" pad="3"/>
<contactref element="MOD1" pad="P$18"/>
<contactref element="MOD1" pad="P$58"/>
</signal>
<signal name="TX">
<contactref element="J2" pad="1"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="RX">
<contactref element="J3" pad="1"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="RS_N">
<contactref element="J2" pad="3"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="RS_P">
<contactref element="J3" pad="3"/>
<contactref element="U6" pad="1"/>
</signal>
<signal name="RS1_N">
<contactref element="U6" pad="7"/>
<contactref element="R12" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="RS1_P">
<contactref element="U6" pad="6"/>
<contactref element="R11" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="IC2" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="IC3" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="KEY_SENSE">
<contactref element="TP7" pad="TP"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="MOD1" pad="P$51"/>
<contactref element="MOD1" pad="P$11"/>
</signal>
<signal name="STATUS">
<contactref element="U7" pad="4"/>
<contactref element="U10" pad="4"/>
<contactref element="U9" pad="4"/>
<contactref element="U8" pad="4"/>
<contactref element="R29" pad="2"/>
<contactref element="TP9" pad="TP"/>
<contactref element="MOD1" pad="P$15"/>
<contactref element="MOD1" pad="P$55"/>
</signal>
<signal name="LIO1">
<contactref element="J4" pad="2"/>
<contactref element="MOD1" pad="P$61"/>
<contactref element="MOD1" pad="P$21"/>
</signal>
<signal name="LIO2">
<contactref element="J5" pad="2"/>
<contactref element="MOD1" pad="P$62"/>
<contactref element="MOD1" pad="P$22"/>
</signal>
<signal name="LIO3">
<contactref element="J6" pad="2"/>
<contactref element="MOD1" pad="P$23"/>
<contactref element="MOD1" pad="P$63"/>
</signal>
<signal name="LIO4">
<contactref element="J7" pad="2"/>
<contactref element="MOD1" pad="P$24"/>
<contactref element="MOD1" pad="P$64"/>
</signal>
<signal name="N$1">
<contactref element="J8" pad="2"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U7" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J4" pad="3"/>
<contactref element="D9" pad="3"/>
<contactref element="R15" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U8" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R16" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="D10" pad="3"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="R17" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="D11" pad="3"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U9" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U10" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R18" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="D12" pad="3"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="J9" pad="2"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J10" pad="2"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="J11" pad="2"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="TP11" pad="TP"/>
<contactref element="MOD1" pad="P$4"/>
<contactref element="MOD1" pad="P$44"/>
</signal>
<signal name="N$27">
<contactref element="TP26" pad="TP"/>
<contactref element="MOD2" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="TP27" pad="TP"/>
<contactref element="MOD2" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="TP28" pad="TP"/>
<contactref element="MOD2" pad="7"/>
</signal>
<signal name="N$30">
<contactref element="TP29" pad="TP"/>
<contactref element="MOD2" pad="8"/>
</signal>
<signal name="N$46">
<contactref element="TP30" pad="TP"/>
<contactref element="MOD2" pad="9"/>
</signal>
<signal name="N$47">
<contactref element="MOD2" pad="11"/>
<contactref element="TP41" pad="TP"/>
</signal>
<signal name="N$48">
<contactref element="TP40" pad="TP"/>
<contactref element="MOD2" pad="12"/>
</signal>
<signal name="N$49">
<contactref element="MOD2" pad="13"/>
<contactref element="TP39" pad="TP"/>
</signal>
<signal name="N$50">
<contactref element="MOD2" pad="14"/>
<contactref element="TP38" pad="TP"/>
</signal>
<signal name="N$51">
<contactref element="MOD2" pad="16"/>
<contactref element="TP36" pad="TP"/>
</signal>
<signal name="N$52">
<contactref element="MOD2" pad="17"/>
<contactref element="TP35" pad="TP"/>
</signal>
<signal name="N$53">
<contactref element="MOD2" pad="18"/>
<contactref element="TP34" pad="TP"/>
</signal>
<signal name="N$54">
<contactref element="MOD2" pad="19"/>
<contactref element="TP33" pad="TP"/>
</signal>
<signal name="N$55">
<contactref element="MOD2" pad="20"/>
<contactref element="TP32" pad="TP"/>
</signal>
<signal name="SWITCHED_PWR">
<contactref element="TP1" pad="TP"/>
<contactref element="J1" pad="J-G12"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U11" pad="7"/>
<contactref element="U11" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="C20" pad="1"/>
<contactref element="U5" pad="8"/>
<contactref element="C19" pad="2"/>
</signal>
<signal name="V+">
<contactref element="C19" pad="1"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="V-">
<contactref element="C22" pad="2"/>
<contactref element="U5" pad="10"/>
</signal>
<signal name="C2-">
<contactref element="U5" pad="15"/>
<contactref element="C28" pad="2"/>
</signal>
<signal name="C2+">
<contactref element="C28" pad="1"/>
<contactref element="U5" pad="16"/>
</signal>
<signal name="C1-">
<contactref element="U5" pad="1"/>
<contactref element="C27" pad="2"/>
</signal>
<signal name="C1+">
<contactref element="U5" pad="2"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U4" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="U4" pad="6"/>
<contactref element="L2" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="D5" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U3" pad="6"/>
<contactref element="D4" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="U3" pad="3"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="U3" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="U4" pad="1"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="SHUTDOWN">
<contactref element="U3" pad="4"/>
<contactref element="U4" pad="4"/>
<contactref element="U11" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="IC2" pad="6"/>
<contactref element="L3" pad="4"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="IC2" pad="7"/>
<contactref element="L3" pad="3"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="IC3" pad="7"/>
<contactref element="L4" pad="3"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="IC3" pad="6"/>
<contactref element="L4" pad="4"/>
<contactref element="D7" pad="2"/>
</signal>
<signal name="KEEP_ALIVE">
<contactref element="U2" pad="1"/>
<contactref element="TP8" pad="TP"/>
<contactref element="MOD1" pad="P$52"/>
<contactref element="MOD1" pad="P$12"/>
</signal>
<signal name="N$56">
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="N$60">
<contactref element="T1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="VGND">
<contactref element="T1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="J-B1"/>
</signal>
<signal name="V_PROT">
<contactref element="Q1" pad="3"/>
<contactref element="C6" pad="+"/>
<contactref element="C9" pad="+"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="J9" pad="1"/>
<contactref element="J10" pad="1"/>
<contactref element="J11" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U11" pad="8"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="J1" pad="J-B2"/>
<contactref element="T1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U10" pad="5"/>
<contactref element="U9" pad="8"/>
<contactref element="U7" pad="5"/>
<contactref element="U8" pad="5"/>
<contactref element="U7" pad="8"/>
<contactref element="U9" pad="5"/>
<contactref element="U8" pad="8"/>
<contactref element="U7" pad="6"/>
<contactref element="U7" pad="7"/>
<contactref element="U8" pad="6"/>
<contactref element="U8" pad="7"/>
<contactref element="U9" pad="6"/>
<contactref element="U9" pad="7"/>
<contactref element="U10" pad="6"/>
<contactref element="U10" pad="7"/>
<contactref element="U10" pad="8"/>
</signal>
<signal name="N$61">
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="SPARE1">
<contactref element="TP3" pad="TP"/>
<contactref element="J1" pad="J-B10"/>
</signal>
<signal name="SPARE2">
<contactref element="TP4" pad="TP"/>
<contactref element="J1" pad="J-B9"/>
</signal>
<signal name="GND">
<contactref element="D6" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
